For 1990-2009 cars

## Door Sill Plate Replacement Sedan

### Removal Procedure

1. Remove the complete door sill plate.

Loosen the 5 clips.

2. Remove the door sill plate upwards.

### Installation Procedure

1. Install the complete door sill plate.
2. Install the 5 clips.

## Door Sill Plate Replacement Coupe

### Removal Procedure

1. Remove the door sill plate.

Release the 5 clips.

2. Remove the door sill plate (1).

### Installation Procedure

1. Install the door sill plate.
2. Install the 5 clips.