For 1990-2009 cars

### Removal Procedure

1. Remove the engine. Refer to Engine Replacement .
2. Remove the manual transmission from the engine. Refer to Transmission Replacement .
3. Remove the automatic transmission from the engine with the torque converter. Refer to Transmission Replacement .
4. Remove the pressure plate and clutch disc. Refer to Clutch, Pressure Plate, and Pilot Bearing Replacement .
5. Remove the flywheel. Refer to Engine Flywheel Replacement .
6. Remove the drive belt. Refer to Drive Belt Replacement .
7. Remove the oil pan. Refer to Oil Pan Replacement .
8. Remove the oil pump module.

| Important: Note the different screw lengths.

• | Remove the 8 bolts (1, 2).

• | Remove the gasket.

9. Identify all the con-rod bearing caps (1).
10. Remove the con-rod bearing caps 1 and 4 (1).

Remove the 4 bolts.

11. Turn the crankshaft through 180 degrees.
12. Remove the con-rod bearing caps 2 and 3 (1).

Remove the 4 bolts.

13. Identify the crankshaft bearing caps.
14. Remove the crankshaft bearing cap (1).

Remove the 10 bolts.

15. Remove the crankshaft.
16. Remove the crankshaft bearing clips.

### Installation Procedure

Important: Inspect the installation position.

1. Install the crankshaft bearing clips.

Oil bearing clips.

2. Install the crankshaft.

Important: Inspect the installation position.

3. Install the crankshaft bearing caps 1-4.

• | Oil bearing clips.

• | Install the 8 bolts.

Notice: Refer to Fastener Notice in the Preface section.

Important: Inspect the installation position.

4. Install the crankshaft bearing cap.

• | Apply the adhesive sealing compound (black) to the grooves of the rear crankshaft bearing cap.

• | Install the 2 bolts.

5. Tighten the crankshaft bearing cap.

Use new bolts.

Tighten
Tighten the 10 bolts to 50 N·m (37 lb ft) plus 45 degrees plus 15 degrees.

Important: Inspect the installation position.

6. Install the con-rod bearing caps 2 and 3.

• | Oil bearing clips.

• | Renew the bolts.

Tighten
Tighten the 4 bolts to 35 N·m (26 lb ft) plus 45 degrees plus 15 degrees.

7. Turn the crankshaft through 180 degrees.

Important: Inspect the installation position.

8. Install the con-rod bearing caps 1 and 4.

• | Oil bearing clips.

• | Install new the bolts.

Tighten
Tighten the 4 bolts to 35 N·m (26 lb ft) plus 45 degrees plus 15 degrees.

9. Replace the crankshaft seal ring (rear). Refer to Crankshaft Rear Oil Seal Replacement .

Important: Note the different screw lengths.

10. Install the oil pump module.

Replace the gasket.

Tighten
Tighten the 8 bolts to 20 N·m (15 lb ft).

11. Seal Ring - Front Crankshaft, Replace. Refer to Crankshaft Front Oil Seal Replacement .
12. Install the oil pan. Refer to Oil Pan Replacement
13. Install the flywheel. Refer to Engine Flywheel Replacement .
14. Install the pressure plate and clutch disk. Refer to Clutch, Pressure Plate, and Pilot Bearing Replacement .
15. Replace the drive belt drive gear.
16. Install the drive belt. Refer to Drive Belt Replacement .
17. Install the automatic transmission in engine with torque converter. Refer to Transmission Replacement .
18. Install the manual transmission. Refer to Transmission Replacement .
19. Install the engine. Refer to Engine Replacement .