For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket.
2. Remove the front floor console. Refer to Front Floor Console Replacement.
3. Remove the door sill plate. Refer to Door Sill Plate Replacement.
4. Remove the rear floor air dust rear footwell (1).
5. Remove the brace, instrument panel (I/P) padding.

• | Remove the left brace (3) when replacing the left air duct for footwell.

• | Remove the 4 bolts.

• | Remove the right brace when replacing the right (2) air duct for footwell.

• | Remove the 2 bolts.

6. Detach and lift the floor covering at front in area or rear air duct for footwell.
7. Remove the air duct rear footwell (1).

Remove the air duct and withdraw to the front.

### Installation Procedure

1. Install the air duct footwell rear.
2. Position and attach floor covering at front in area or rear air duct for footwell.
3. Install brace, instrument panel padding.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the left brace when replacing the left air duct for footwell.

Tighten
Tighten the 4 bolts to 13 N·m (113 lb in).

5. Install the right brace when replacing the right air duct for footwell.

Tighten
Tighten the 2 bolts to 13 N·m (113 lb in).

6. Install the air distribution rear footwell.
7. Insert the air distribution footwell at top and at the bottom slide onto the air duct footwell rear.
8. Install the door sill plate. Refer to Door Sill Plate Replacement.
9. Install the front floor console. Refer to Front Floor Console Replacement.
10. Install the front seat. Refer to Front Seat Replacement - Bucket.