For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Inflator Module Handling and Storage Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Wait 1 minute for airbag to deactivate.

Important: Ensure that the retaining wire is not bent.

3. Remove the airbag.

• | Turn the steering wheel 90 degrees (I).

• | Push the retaining wire in the direction of the steering column using a small screwdriver in the service opening (II) and remove the airbag module.

• | Release and disconnect the wiring harness plug.

### Installation Procedure

1. Install the airbag.

• | Connect and latch the wiring harness plug.

• | Install the 2 clips.

2. Perform a readiness inspection.
3. Connect the battery.
4. For programming procedures, refer to Control Module References .