For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door trim panel.

Remove the access panel with a plastic wedge.

Important: The moveable handle part must now be secured in pulled position.

2. Remove the rear door fixed handle part.

• | Pull out and hold the moveable handle part (I).

• | Turn the bolt (II) left until it stops.

• | Remove the fixed handle part with lock cylinder (IV).

3. Remove the door handle.

Pull back the moveable handle part (III) to remove.

### Installation Procedure

1. Install the door handle.

Install the moveable handle part into the door panel.

Important: Hold the moveable handle part in place while turning the bolt.

2. Install the rear door fixed handle part.

• | Install the fixed handle part.

• | Turn the bolt right until it stops.

• | Insert the cover cap.

3. Install the front side door trim panel.