For 1990-2009 cars

### Removal Procedure

1. Remove the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
2. Remove the sensor mat, seat belt fastened detection.

Remove the sensor mat (1) and replace.

### Installation Procedure

1. Install the sensor mat, seat belt fastened detection.

Install the sensor mat with adhesive.

2. Install the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .