For 1990-2009 cars

### Removal Procedure

1. Remove the repeater lamp on the right side.

Press the repeater lamp in the direction of the arrow using a plastic wedge, and remove.

2. Disconnect the repeater lamp.

Disconnect the wiring harness plug (1).

3. Remove the repeater lamp on the left side.

Press the repeater lamp in direction of the arrow using a plastic wedge, and remove.

4. Disconnect the repeater lamp.

Disconnect the wiring harness plug (1).

5. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Connect the wiring harness plug for the repeaters.
3. Install the repeater lamp.