For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) compartment.

1.1. | Remove the 4 bolts (1).

1.2. | Disconnect the wiring harness plug.

2. Remove the floor air outlet duct.

Remove the body-bound rivet (2).

### Installation Procedure

1. Install the floor air outlet duct.

Install the body-bound rivet.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the I/P compartment.

Install the 4 bolts

Tighten
Tighten the 4 bolts to 4 N·m (35 lb in).

3. Connect the wiring harness plug.