For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.

Remove the positive and negative cables.

2. Wait 1 minute for the airbag to deactivate.
3. Remove the battery.

Remove the bolt.

4. Remove the airbag sensor.

• | Remove the 2 bolts (1).

• | Disconnect the wiring harness plug and remove the sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the airbag sensor.

Insert the sensor and connect the wiring harness plug.

Tighten
Tighten the 2 bolts to 6 N·m (53 lb in).

2. Install the battery.
3. Connect the battery.

Tighten
Tighten the bolt to 5 N·m (44 lb in).

4. Perform the readiness inspection.
5. For programming procedures, refer to Control Module References .