For 1990-2009 cars

### Removal Procedure

1. Position the seat to the most forward position.
2. Remove the height adjuster panel.

Release with a plastic wedge.

3. Remove the height adjuster.

Remove the 2 bolts (1) and the lever.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the height adjuster.

Tighten
Tighten the 2 bolts to 35 N·m (26 lb ft).

2. Install the height adjuster panel.

Clip in panel.

3. Reposition the seat to the original position.