For 1990-2009 cars

#### Special Tools

BO-46862 Radio Removal Tool

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the radio.

2.1. | Remove the radio using BO-46862 .

2.2. | Push the removal bracket into the openings (arrows) until it engages, press outwards and withdraw radio.

2.3. | Disconnect the antenna cable (1).

2.4. | Disconnect the wiring harness plug (2).

2.5. | Release and disconnect the wiring harness plug.

3. Disconnect the heating control.

3.1. | Release the 2 clips at top (1).

3.2. | Disconnect the 2 wiring harness plugs (2).

3.3. | Release and disconnect the wiring harness plug.

### Installation Procedure

1. Connect the heating control.

1.1. | Install the 2 clips.

1.2. | Connect the 2 wiring harness plugs.

2. Install the radio.

2.1. | Connect the antenna cable.

2.2. | Connect the wiring harness plug.

3. Connect the battery.
4. For programming procedures, refer to Control Module References .