For 1990-2009 cars

### Removal Procedure

1. Lower the molded headlining. Refer to Headlining Trim Panel Replacement .
2. Remove the rear water drain hose.

• | Remove the water drain hose from the sunroof.

• | Remove the outer run-off in the direction of the vehicle interior.

### Installation Procedure

1. Install the rear water drain hose.

Insert the water drain hose in the roof frames and attach to the sunroof.

2. Install the molded headlining. Refer to Headlining Trim Panel Replacement .