For 1990-2009 cars

### Removal Procedure

1. Remove the radiator grille.

• | Remove the 4 body-bound rivets.

| Release from the front paneling upward.

• | Release the 6 clips.

2. Release the solvent container at the top front.

Remove the bolt (1).

3. Release the solvent container at the base.

Remove the 2 bolts (2).

Note: Drain the washer solvent into a suitable container.

4. Remove the hoses and wiring harness plugs.

| Note: Depending on vehicle design.

• | Disconnect the 3 wiring harness plugs (1, 2).

| Note: Depending on vehicle design.

• | Disconnect the 3 hoses (3, 4).

• | Unclip the 3 hoses.

• | Remove the solvent container downward.

• | Remove the wiring harness.

Note: Depending on vehicle design.

5. Remove the attachment.

• | Remove the pump for the front and rear screens.

• | Remove the pump for the headlamp washer system.

• | Remove the fill level sensor.

• | Bring the pin to vertical position for removal.

### Installation Procedure

Note: Depending on vehicle design.

1. Install the attachments.

• | Install the pump for the front and rear screens.

• | Install the pump for the headlamp washer system.

• | Install the fill level sensor.

2. Install the solvent container at the base.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the cable tie.

Tighten
Tighten the 2 screws to 3.5 N·m (31 lb in).

Note: Depending on vehicle design.

4. Install the hoses and the wiring harness plugs.

• | Connect the 3 wiring harness plugs.

• | Connect the 3 hoses.

5. Install the solvent container at the top front.

Tighten
Tighten the bolt to 3.5 N·m (31 lb in).

6. Install the radiator grille.

• | Insert the 4 body-bound rivets.

• | Install the front paneling downward.

• | Clip in the 6 clips.

7. Top up the washer fluid.