For 1990-2009 cars

Condition | Action
--- | ---
DEFINITION: Transmission overheats
Low fluid level | Inspect for leaks and repair as necessary.
Incorrect fluid | Replace the fluid with the correct fluid
Fluid Filter (42) is restricted |

• | Diagnose the cause for the filter restriction and repair as needed.

• | Replace the fluid filter (42) and fluid.

Restricted Oil Cooler Lines |

• | Inspect for bent or kinked pipes

• | Inspect for pinched or kinked hoses

• | Inspect for cracks or signs of hose overheating that may cause delamination of the hose

• | Replace faulty oil cooler lines

Internal oil cooler restriction | Replace radiator assembly and fluid.