For 1990-2009 cars

#### Special Tools

J 39637 /KM-6626 Wiper Arm Puller

### Removal Procedure

Remove the windshield wiper arm.

• | Remove the 2 covers.

• | Remove the 2 nuts (2).

• | Pull off the wiper arm using J 39637 /KM-6626.

• | Remove the 2 washers.

### Adjustment Procedure

Measure the point for the windshield wiper arms.

The upper edge of the water deflector (rubber lip) to wiper arm attachment point

Important: Move the wiper arm to basic setting.

1. Driver side approximately 5.5 cm (2.17 in)
2. Passenger side approximately 5.5 cm (2.17 in)

### Installation Procedure

1. Install the windshield wiper arm.

Notice: Refer to Fastener Notice in the Preface section.

• | Install the washer.

Tighten
Tighten the windshield wiper arm nut to 17 N·m (13 lb ft).

• | Install the cover.

2. Adjust the windshield wiper arms. Refer to Windshield Wiper Arm Adjustment .