For 1990-2009 cars

### Removal Procedure

1. Remove the control valve body cover. Refer to Control Valve Body Cover Replacement.
2. Remove the 2-3 shift solenoid valve bolt (314) and the 2-3 shift solenoid valve (313).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the 2-3 shift valve solenoid valve (313) and the bolt (314).

Tighten
Tighten the bolt to 5.9-7.4 N·m (51-66 lb in).

2. Install the control valve body cover. Refer to Control Valve Body Cover Replacement.