For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.
2. Remove the instrument panel (I/P) trim panel. Refer to Instrument Panel Trim Panel Replacement.
3. Remove the front floor console. Refer to Front Floor Console Replacement.
4. Remove the I/P padding wiring harness (LAD).
5. Remove the I/P padding wiring harness (RHD).

### Installation Procedure

1. Install the I/P padding wiring harness.
2. Install the I/P trim panel. Refer to Instrument Panel Trim Panel Replacement.
3. Install the front floor console. Refer to Front Floor Console Replacement.
4. Connect the battery.
5. For programming procedures, refer to Control Module References.