For 1990-2009 cars

1. Clean the exhaust manifold sealing surface.
2. Install a NEW exhaust manifold gasket to the exhaust manifold.
3. Install the exhaust manifold.

Notice: Refer to Fastener Notice in the Preface section.

4. Install NEW exhaust manifold nuts (1).

Tighten
Tighten the 9 nuts to 20 N·m (15 lb ft).

5. Install the exhaust manifold heat shield (3).
6. Install the wiring harness bracket (2) and bolt (1).

Tighten
Tighten the bolt to 15 N·m (11 lb ft).