For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) ashtray. Refer to Instrument Panel Ashtray Replacement.
2. Remove the ashtray bulb.

• | Release the retaining lug (1).

• | Remove the bulb and the holder.

• | Remove the bulb.

### Installation Procedure

1. Insert the ashtray bulb.

• | Place the bulb into the holder.

• | Install the holder.

2. Install the I/P ashtray. Refer to Instrument Panel Ashtray Replacement.