For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
2. Remove the impact bar (1).

• | Remove the 8 nuts (2 and 4).

• | Remove the 2 lock nuts (3).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: Use NEW nuts.

1. Install the rear impact bar.

Tighten
Tighten the 8 nuts to 20 N·m (15 lb ft).

2. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.