For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery.
2. Wait 1 minute for the airbag to deactivate.
3. Remove the front floor console. Refer to Front Floor Console Replacement.
4. Remove the airbag control unit.

Remove the 3 nuts (1) and remove the control unit.

5. Loosen the airbag wiring harness.

Release the 2 wiring harness plugs and disconnect.

### Installation Procedure

1. Fasten the airbag wiring harness.

Connect and latch the wiring harness plug.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the airbag control unit.

• | Connect 2 wiring harness plugs.

Tighten
Tighten the 3 nuts to 10 N·m (89 lb in).

3. Install the front floor console. Refer to Front Floor Console Replacement
4. Connect the battery.

Note: When replacing the control unit, after installing the control unit, program with a scan tool.

5. For programming procedures, refer to Control Module References.