For 1990-2009 cars

### Removal Procedure

1. Remove the heating/air conditioning control. Refer to Heater and Air Conditioning Control Replacement.
2. Remove the accessory panel on instrument panel (I/P) padding.

2.1. | Remove the 2 bolts (1).

2.2. | Remove the panel.

2.3. | Disconnect the wiring harness plug (2).

2.4. | Release and disconnect the wiring harness plug.

3. Remove the accessory panel.

Release the 2 locks (1).

### Installation Procedure

1. Install the accessory panel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the accessory panel on I/P padding.

• | Connect the wiring harness plug.

• | Install the accessory trim panel.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

3. Install heating/air conditioning unit control. Refer to Heater and Air Conditioning Control Replacement.