For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

Note: When replacing the control unit, before removing the control unit, carry out a "Reset" using Tech 2. For reprogramming procedures, refer to Control Module References.

1. Disconnect the battery.
2. Remove the steering wheel. Refer to Steering Wheel Replacement.
3. Remove the lower steering column panel.

• | Remove the 5 bolts (arrows).

• | Remove the ignition lock panel (1).

4. Remove the column integration module (CIM).

• | Remove the 3 bolts (1).

• | Disconnect the wiring harness holder (arrow).

• | Release the wiring harness plug (2) and disconnect.

5. Remove the theft deterrent module.

• | Release the 2 clips (1, 2).

• | Remove the module.

### Installation Procedure

1. Install the theft deterrent module.

Install the 2 clips.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CIM.

• | Connect and lock the wiring harness plug.

• | Connect the wiring harness holder.

Tighten
Tighten the 3 bolts to 2.5 N·m (22 lb in).

3. Install the lower steering column panel.

Install the ignition lock panel.

Tighten
Tighten the 5 screws to 2.5 N·m (22 lb in).

4. Install the steering wheel. Refer to Steering Wheel Replacement.
5. For reprogramming procedures, refer to Control Module References.