For 1990-2009 cars

### Removal Procedure

1. Open the hood.

Warning: Refer to Battery Disconnect Warning in the Preface section.

2. Disconnect the battery.

• | Remove the negative connection from the ground terminal.

• | Loosen the nut.

3. Remove the drive belt. Refer to Drive Belt Replacement.
4. Disconnect the generator from the power supply.

• | Disconnect the generator from the power supply.

• | Remove the 2 nuts (1, 2).

5. Remove the generator.

Remove the 2 bolts (3, 4).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the generator.

Tighten
Tighten the 2 bolts to 35 N·m (25 lb ft).

2. Install the wiring harness to the generator.

Tighten
Tighten the 2 nuts to 7 N·m (62 lb in).

3. Install the drive belt. Refer to Drive Belt Replacement.
4. Connect the battery.

Install the negative connection to the ground terminal.

Tighten
Tighten the nut to 5 N·m (44 lb in).

5. For programming procedures, refer to Control Module References.
6. Close the hood.