For 1990-2009 cars

### Removal Procedure

1. Remove the lower steering column paneling.

• | Remove the 5 bolts (arrows).

• | Remove the ignition lock panel (1).

2. Remove the lock cylinder.

• | Ignition key to position I.

• | Remove the lock cylinder with a suitable tool (screwdriver) (1).

• | Remove the lock cylinder (arrow).

### Installation Procedure

1. Install the lock cylinder.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lower steering column paneling.

Tighten
Tighten the 5 screws to 1 N·m (9 lb in).

3. Install the 2 panels.