For 1990-2009 cars

Condition | Action
--- | ---
DEFINITION: Engagement time from park or neutral to drive is not within specifications
Fluid level low and/or contaminated with water or engine coolant |

• | Perform Transmission Fluid Check .

• | If contaminated with engine coolant replace transmission.

Fluid is burnt |

• | Inspect transmission oil cooler system for restricted or kinked lines.

• | Flush system. Refer to Transmission Fluid Cooler Flushing and Flow Test .

Unit filled with wrong type of fluid | Drain and fill with proper type of fluid.
Input Speed Sensor (76) |

• | Perform electrical function check on the input speed sensor (76).

• | Replace input speed sensor (76) if failed.

Valve body (39) | Replace valve body (39).
Internal transmission part failure |

• | Disassemble the transmission and inspect the following:

- | Clutch assemblies, O-rings cut or damaged, clutch disc failure

- | Fluid pump wore or scored components

• | Replace transmission if any parts are faulty.