For 1990-2009 cars

## Sunshade Replacement Visor Cover

### Removal Procedure

1. Remove the sunshade cover (1).
2. Remove the 2 clips.

### Installation Procedure

1. Install the sunshade cover.
2. Install the 2 clips.

## Sunshade Replacement Visor

### Removal Procedure

1. Open the liftgate.
2. Remove the lock trim panel.

2.1. | Release the clips.

2.2. | Remove the bolt.

3. Remove the luggage shade retainers for the liftgate garnish molding (3) left side.
4. Remove the upper liftgate garnish molding (2) left side.

Release the 4 clips.

5. Remove the luggage shade retainers for the liftgate garnish molding (3) right side.
6. Remove the upper liftgate garnish molding (2) right side.

Release the 4 clips.

7. Remove the lower liftgate trim panel.

Release the 8 clips.

8. Remove the liftgate applique.

8.1. | Disconnect the wiring harness plug.

8.2. | Remove the 6 nuts (1).

8.3. | Remove the liftgate applique (arrows).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the liftgate applique.

Connect the wiring harness plug.

Tighten
Tighten the 6 nuts to 3 N·m (26 lb in).

2. Install the lower liftgate trim panel.
3. Install the lock trim panel.

Tighten
Tighten the bolt to 5 N·m (44 lb in).

4. Install the liftgate garnish moldings, right side.
5. Install the luggage shade retainers for the garnish moldings, right side.
6. Install the garnish moldings, left side.
7. Install the luggage shade retainers for the garnish moldings, left side.
8. Close the liftgate.