For 1990-2009 cars

### Removal Procedure

1. Remove the upper extension trim panel.

Release the 3 clips.

2. Remove the front door outer mirror.

Remove the 3 bolts.

3. Remove the protective cover (1) from the outer mirror inner paneling (2).

Remove the protective cover.

### Installation Procedure

1. Install the protective cover.
2. Install the protective cover in the outer mirror inner paneling.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front door outer mirror.

Tighten
Tighten the 3 bolts to 5 N·m (44 lb in).

4. Install the upper extension trim panel.

Install the 3 clips.