For 1990-2009 cars

### Removal Procedure

1. Remove the panel for the microphone (2) and the panel for the sliding sun roof control unit (3) using a suitable tool (flat-bladed tool).
2. Remove the lens from the interior lamp (1).
3. Remove the front interior lamp holder.

• | Remove the 2 bolts (1).

• | Remove the holders (4) all around.

• | Disconnect the wiring harness holder (2).

• | Disconnect the wiring harness plug (3).

4. Remove the ultrasound sensor.

• | Disconnect the compact plug (1).

• | Disconnect the wiring harness at the compact plug (arrow).

• | Remove the panel with the ultrasonic sensors (2).

5. Remove the necessary lamps.

Remove the 2 bulbs.

### Installation Procedure

1. Install the necessary lamps.

Install the 2 bulbs.

2. Install the ultrasound sensors.

• | Install the panel with the ultrasound sensors.

• | Insert the wiring harness in the compact plug and lock.

• | Connect in the compact plug.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the front interior lamp holder.

• | Connect the wiring harness plug.

• | Connect the wiring harness holder.

• | Connect the holders all around.

Tighten
Tighten the 2 screws to 1.5 N·m (13 lb in).

4. Install the lens for the interior lamp.

Install the 4 clips.

5. Install the microphone panel and the panel for the sliding sun roof control unit.

Install the 2 panels.