For 1990-2009 cars

Condition | Action
--- | ---
DEFINITION: When shift lever is moved the transmission will not respond.
Park/neutral position switch (72) |

• | Inspect the park/neutral position switch (72) for proper alignment.

• | Adjust the park/neutral position switch (72) for proper alignment.

Shift cable adjustment |

• | Inspect shift cable to ensure transmission is shifting in the proper shift positions.

• | Adjust shift cable if out of adjustment.

Internal transmission failure |

• | Disassemble the transmission and inspect the following:

- | Manual shift lever and the manual shift valve for proper operation

- | Broken gears or shafts

• | If failed components, replace transmission assembly.