For 1990-2009 cars

## Liftgate Trim Panel Replacement Sedan

### Removal Procedure

1. Remove the lock cover trim panel.

• | Release the clip.

• | Remove the bolt.

2. Remove the upper garnish molding (2)--left side.

• | Remove the luggage shade bracket (3).

• | Release the 4 clips.

3. Remove the upper garnish molding (2)--right side.

• | Remove the luggage shade bracket (3).

• | Release the 4 clips.

4. Remove the liftgate trim panel (1).

Release the 8 clips.

### Installation Procedure

1. Install the liftgate trim panel.

Install the 8 clips.

2. Install the upper garnish molding--left side.

Install the 4 clips.

3. Install the upper garnish molding--right side.

Install the 4 clips.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the lock cover trim panel.

Install the clip.

Tighten
Tighten the bolt.

## Liftgate Trim Panel Replacement Coupe

### Removal Procedure

1. Support the luggage shade from the liftgate.

Disconnect the 2 retaining cords.

2. Remove the upper right and left liftgate garnish molding (1).

• | Remove the 2 luggage shade retainers (2).

• | Release the 6 clips.

3. Remove the liftgate lock cover trim panel.

• | Remove the body-bound rivet.

• | Release the 3 inner handle cups.

4. Remove the liftgate trim panel.

Release the 8 clips (1).

### Installation Procedure

1. Install the liftgate trim panel.

Install the 8 clips.

2. Install the liftgate lock cover trim panel.

• | Install the 3 inner handle cups.

• | Install the body-bound rivet.

3. Install the upper right and left liftgate garnish moldings.

• | Install the 6 clips.

• | Install the 2 luggage shade retainers.

4. Install the luggage shade to the liftgate.

Install the 2 retaining cords.