For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Carrier Bolt | 15 N·m | 11 lb ft
Battery Holder Bolt | 7 N·m | 62 lb in
Battery Shield Bolt | 10 N·m | 89 lb in
Generator Bolt | 35 N·m | 25 lb ft
Ground Cable to Starter Nut | 12.5 N·m | 110 lb in
Ground Connection to Ground Terminal Nut | 12.5 N·m | 110 lb in
Ground Terminal Nut | 5 N·m | 44 lb in
Intake Manifold Bracket Bolt | 8 N·m | 70 lb in
Starter Bolt | 25 N·m | 18 lb ft
Wiring Harness to Starter Nut | 12.5 N·m | 110 lb in
Wiring Harness to Generator Nut | 7 N·m | 62 lb in