For 1990-2009 cars

### Removal Procedure

Caution: Refer to Express Down Feature Caution in the Preface section.

1. Remove the front side door window regulator. Refer to Front Side Door Window Regulator Replacement .
2. Remove the motor from the linkage.

Remove the 3 bolts (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the motor to the linkage.

Tighten
Tighten the 3 bolts to 3.5 N·m (32 lb in).

2. Install window lifter. Refer to Front Side Door Window Regulator Replacement .