For 1990-2009 cars

### Removal Procedure

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

Notice: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.

Remove the strut.

• | Support the liftgate.

• | Open the retaining clips.

• | Remove the strut.

### Installation Procedure

Install the strut.

• | Support the liftgate.

• | Install the strut.