For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console.

Disconnect the 8 clips and remove the storage compartment.

2. Loosen the front floor console.

2.1. | Place both of the seats in the most forward position.

2.2. | Remove the nut (2).

2.3. | Remove the 2 bolts (1).

3. Disconnect the hand brake molding.
4. Loosen the front floor console and middle.

4.1. | Position both seats to the rear-most position.

4.2. | Remove the 2 bolts (1), front.

4.3. | Remove the Tech2 connection molding.

4.4. | Remove the middle bolt (2).

5. If equipped with storage compartment, remove the storage compartment then remove the ashtray.

Disconnect the 2 wiring harness plug.

6. Loosen the front floor console upper front.

Remove the 2 bolts (2).

7. Remove the console shift level bezel.

Remove the 2 bolts (1).

Important: Carefully take out the front floor console to the rear.

8. Remove the front floor console.
9. If necessary, remove the cover (1) from console retaining bolt.

### Installation Procedure

1. Position the front floor console.

Slide the console in the front-most guide (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the gear .

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

3. Fasten the console, upper front.

Tighten
Tighten the 2 bolts to 2.5 N·m (22 lb in).

4. If equipped with storage compartment, install the storage compartment and then Install the ashtray.

Connect the 2 wiring harness plugs.

5. Fasten the console front and center.

• | Position both seats in rear-most position.

Tighten
Tighten the 3 bolts to 2.5 N·m (22 lb in).

• | Install the Tech2 connection molding.

6. Install the hand brake molding.
7. Install the console, rear.

Position both seats to the most forward position.

Tighten

• | Tighten the nut to 2.5 N·m (22 lb in).

• | Tighten the 2 bolts to 2.5 N·m (22 lb in).

8. Install the console storage compartment, rear .

Install the 8 clips.