For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: Only upon replacement of air inlet actuator.

1. Disconnect the battery.
2. Remove the instrument panel (I/P) compartment.

2.1. | Remove the 4 bolts (1).

2.2. | Disconnect the wiring harness plugs.

3. Remove the recirculation actuator (1).

• | Remove the 3 bolts.

• | Disconnect the wiring harness plug (2).

• | Release and disconnect the wiring harness plug.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: The recirculation actuator can only be fitted in one position and is self-calibrating.

1. Install the recirculation actuator.

Tighten
Tighten the 3 bolts to 5 N·m (44 lb in).

2. Connect the wiring harness plug.
3. Install the I/P compartment.
4. Connect the wiring harness plug.

Tighten
Tighten 4 bolts to 4 N·m (35 lb in).

Important: Only upon replacement of air inlet actuator.

5. Connect the battery.
6. For programming procedures, refer to Control Module References .
7. Perform the function inspection.