For 1990-2009 cars

### Removal Procedure

1. Lower the molded headlining. Refer to Headlining Trim Panel Replacement .
2. Remove the power sunroof motor.

2.1. | Remove the 3 bolts (1).

2.2. | Disconnect the wiring harness plug (2).

### Installation Procedure

1. Install the power sunroof motor.

Notice: Refer to Fastener Notice in the Preface section.

2. Connect the wiring harness plug.

Tighten
Tighten the 3 bolts to 7 N·m (62 lb in).

3. Install the molded headlining. Refer to Headlining Trim Panel Replacement .

Important: Open and close the sliding sunroof fully.

4. For programming procedures, refer to Control Module References .