For 1990-2009 cars

### Removal Procedure

1. Move the front seat to the rearmost position.
2. Remove the stoplamp switch.

• | Remove the switch fuse (3) in the direction of the arrow.

• | Remove the stoplamp switch.

• | Disconnect the 2 retaining lugs (2).

• | Disconnect the wiring harness plug (1).

### Installation Procedure

1. Install the stoplamp switch.

• | Connect the wiring harness plug.

• | Install and secure the stoplamp switch.

2. Reposition the front seat.