For 1990-2009 cars

#### Special Tools

• | J 39400-A Halogen Leak Detector

• | J 46246 Valve Core Tool

### Removal Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the service port valve core using J 46246 or equivalent.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the service port valve core using J 46246 or equivalent.

Tighten
Tighten the service port valve core to 2.5 N·m (22 lb in).

2. Evacuate and charge the refrigerant system. Refer to Refrigerant Recovery and Recharging.
3. Leak test the fittings using the J 39400-A .