For 1990-2009 cars

### Removal Procedure

1. Remove the ambient light sensor panel (1).

Release the ambient light sensor panel using a plastic wedge.

2. Remove the ambient light sensor (2).

Remove the ambient light sensor from panel.

Important: Secure the wiring harness plug from falling into the installation opening.

3. Disconnect the wiring harness plug (3).

Release and disconnect the wiring harness plug.

### Installation Procedure

1. Connect the wiring harness plug.
2. Install the ambient light sensor.

Install the ambient light sensor into the panel.

3. Install the ambient light sensor panel.

Install the panel with ambient light sensor.