For 1990-2009 cars

### Removal Procedure

1. Lower the molded headlining. Refer to Headlining Trim Panel Replacement.
2. Remove the front water drain hose actuation unit.

Remove the 2 hoses.

3. Remove the rear water drain hose actuation unit.

Remove the 2 hoses.

4. Disconnect the front wiring harness actuation unit.

Disconnect the 2 wiring harness plugs.

5. Release the sunroof module assembly.

Remove the 20 screws.

6. Remove the sunroof module assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Insert the sunroof module assembly.

Fasten with 3 screws.

2. Install the sunroof module assembly.

Tighten
Tighten the 20 screws to 5 N·m (44 lb in).

3. Connect the front wiring harness actuation unit.

Connect the 2 wiring harness plugs.

4. Install the rear water drain hose actuation unit.

Connect the 2 hoses.

5. Install the front water drain hose actuation unit.

Connect the 2 hoses.

6. Install the molded headlining. Refer to Headlining Trim Panel Replacement.