For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Important: When replacing the control unit, before removing the control unit, carry out a "Reset" using Tech 2. For reprogramming procedures, refer to Control Module References .

1. Disconnect the battery.
2. Remove the steering wheel. Refer to Steering Wheel Replacement .
3. Remove the lower steering column panel.

• | Remove the 5 bolts (arrows).

• | Remove the ignition lock panel (1).

4. Remove the column integration module (CIM).

• | Remove the 3 bolts (1).

• | Disconnect the wiring harness holder (arrow).

• | Release the wiring harness plug (2) and disconnect.

5. Remove the theft deterrent module.

• | Release the 2 clips (1, 2).

• | Remove the module.

### Installation Procedure

1. Install the theft deterrent module.

Install the 2 clips.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CIM.

• | Connect and lock the wiring harness plug.

• | Connect the wiring harness holder.

Tighten
Tighten the 3 bolts to 2.5 N·m (22 lb in).

3. Install the lower steering column panel.

Install the ignition lock panel.

Tighten
Tighten the 5 screws to 2.5 N·m (22 lb in).

4. Install the steering wheel. Refer to Steering Wheel Replacement .
5. For reprogramming procedures, refer to Control Module References .