For 1990-2009 cars

### Removal Procedure

Warning: Refer to Express Down Feature Warning in the Preface section.

1. Remove the front side door window regulator. Refer to Front Side Door Window Regulator Replacement.
2. Remove the motor from the linkage.

Remove the 3 bolts (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the motor to the linkage and tighten the 3 bolts to 3.5 N·m (32 lb in).
2. Install window lifter. Refer to Front Side Door Window Regulator Replacement.