For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet screen. Refer to Air Inlet Screen Replacement .
2. Remove the bolts (1) securing the windshield wiper transmission to the vehicle.
3. Disconnect the electrical connections to the windshield wiper motor.
4. Remove the windshield wiper transmission assembly from the vehicle.
5. Remove the windshield wiper motor from the windshield wiper transmission. Refer to Windshield Wiper System Module Replacement .

### Installation Procedure

1. Install the windshield wiper motor to the windshield wiper transmission. Refer to Windshield Wiper System Module Replacement .
2. Position the windshield wiper transmission assembly to the vehicle.
3. Connect the electrical connections to the windshield wiper motor.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the windshield wiper transmission bolts (1).

Tighten
Tighten the bolts to 7.5 N·m (66 lb in).

5. Install the air inlet screen. Refer to Air Inlet Screen Replacement .