For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door window channel. Refer to Rear Side Door Window Channel Replacement .
2. Remove the rubber seal (1) for the fixed window.

Remove from the window channel.

### Installation Procedure

1. Install the rubber seal for fixed window.

Insert into the window channel.

2. Install the rear side door window channel. Refer to Rear Side Door Window Channel Replacement .