For 1990-2009 cars

### Removal Procedure

1. Remove the fluid filter bolt (1) and tube (2).
2. Remove the seal (3) from the fluid filler tube.

### Installation Procedure

1. Install a NEW seal (3) on the fluid filler tube (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fluid filler tube and push fluid filler tube into the transmission as far as the stop.

Tighten
Tighten the bolt (1) to 60 N·m (44 lb ft).

3. Check and add fluid. Refer to Transmission Fluid Check .