For 1990-2009 cars

#### Fastener Tightening Specifications

Description of Usage | Ref No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
2-3 Shift Solenoid Valve Assembly Bolt | 314 | 1 | M5x10 mm | 6.7 N·m | 59 lb in
Apply Tube Retainer Bolt | 50 | 1 | M6x12 mm | 5.4 N·m | 48 lb in
Control Valve Body Bolt | 281 | 5 | M6x20 mm | 10 N·m | 89 lb in
Control Valve Body Bolt | 282 | 1 | M6x76 mm | 10 N·m | 89 lb in
Control Valve Body Bolt | 283 | 1 | M6x55 mm | 10 N·m | 89 lb in
Control Valve Body Bolt | 284 | 1 | M6x12 mm | 10 N·m | 89 lb in
Control Valve Body Bolt | 300 | 1 | M5x75 mm | 6.7 N·m | 59 lb in
Control Valve Body Cover Bolt | 291 | 4 | M8x38-S mm | 24 N·m | 18 lb ft
Control Valve Body Cover Bolt | 292 | 2 | M8x72 mm | 24 N·m | 18 lb ft
Control Valve Body Cover Bolt | 293 | 2 | M8x90 mm | 24 N·m | 18 lb ft
Control Valve Body Cover Bolt | 294 | 1 | M8x25 mm | 24 N·m | 18 lb ft
Control Valve Body Cover Bolt | 295 | 3 | M8x60 mm | 24 N·m | 18 lb ft
Control Valve Body Cover Bolt | 296 | 1 | M8x106.5 mm | 24 N·m | 18 lb ft
Control Valve Body Fluid Passage Bolt | 33 | 1 | M6x50 mm | 10 N·m | 89 lb in
Control Valve Body Fluid Passage Bolt | 34 | 1 | M6x20 mm | 10 N·m | 89 lb in
Front Control Valve Body Cover Bolt | 351 | 4 | M5x40 mm | 6.7 N·m | 59 lb in
Front Control Valve Body Cover Bolt | 352 | 2 | M5x75 mm | 6.7 N·m | 59 lb in
Front Control Valve Body Cover Bolt | 353 | 2 | M5x12 mm | 6.7 N·m | 59 lb in
Front Differential Transfer Drive Gear Assembly Bearing Retainer Bolt | 807 | 1 | M8x20 mm | 13 N·m | 115 lb in
Front Valve Body Bolt | 355 | 2 | M5x54 mm | 6.7 N·m | 59 lb in
Front Valve Body Bolt | 356 | 1 | M5x16 mm | 6.7 N·m | 59 lb in
Line Pressure Control Solenoid Valve Retainer Bolt | 343 | 1 | M5x10 mm | 6.7 N·m | 59 lb in
Lockup Solenoid Clamp Bolt | 304 | 1 | M5x16 mm | 6.7 N·m | 59 lb in
Lube Fluid Pipe Retainer Bolt | 804 | 1 | M6x12 mm | 5.4 N·m | 48 lb in
Manual Shaft Detent Spring Bolt | 712 | 2 | M6x14 mm | 10 N·m | 89 lb in
Manual Shift Shaft Detent Lever Bolt | 715 | 1 | M6x14 mm | 10 N·m | 89 lb in
Manual Shift Shaft Detent Lever Bolt | 718 | 1 | M6x23 mm | 10 N·m | 89 lb in
Manual Shift Shaft Retaining Nut | 69 | 1 | -- | 6.9 N·m | 61 lb in
Middle Control Valve Body Bolt | 365 | 1 | M5x16 mm | 6.7 N·m | 59 lb in
Middle Control Valve Body Bolt | 366 | 2 | M5x38 mm | 6.7 N·m | 59 lb in
No. 2 Rear Control Valve Body Bolt | 362 | 3 | M5x16 mm | 6.7 N·m | 59 lb in
No. 2 Rear Control Valve Body Bolt | 363 | 2 | M5x50 mm | 6.7 N·m | 59 lb in
Park/Neutral Position Switch Bolt | 71 | 2 | M8x26 mm | 25 N·m | 18 lb ft
Rear Valve Body Cover No. 1 Bolt | 437 | 6 | M6x12 mm | 10 N·m | 89 lb in
Rear Valve Body Cover No. 1 Bolt | 443 | 5 | M6x12 mm | 10 N·m | 89 lb in
Rear Valve Body to No. 2 Rear Valve Body Bolt | 357 | 4 | M5x16 mm | 6.7 N·m | 59 lb in
Rear Valve Body to No. 2 Rear Valve Body Bolt | 358 | 1 | M5x38 mm | 6.7 N·m | 59 lb in
Shift Solenoid Valve Assembly Bolt | 315 | 1 | M5x10 mm | 6.7 N·m | 59 lb in
Torque Converter Housing Bolt | 801 | 2 | M8x39 mm | 30 N·m | 22 lb ft
Torque Converter Housing Bolt | 802 | 11 | M8x30 mm | 30 N·m | 22 lb ft
Torque Converter Housing Bolt | 813 | 2 | M8x25-S mm | 30 N·m | 22 lb ft
Transmission Case Cover Bolt | 20 | 10 | M8x25 mm | 25 N·m | 18 lb ft
Transmission Fluid Baffle Bolt | 45 | 2 | M6x12 mm | 5.4 N·m | 48 lb in
Transmission Fluid Baffle Bolt | 810 | 3 | M6x12 mm | 5.4 N·m | 48 lb in
Transmission Fluid Drain Plug | 819 | 1 | -- | 39 N·m | 29 lb ft
Transmission Fluid Pump Cover Bolt | 192 | 8 | M6x18 mm | 10 N·m | 89 lb in
Transmission Fluid Pump to Case Bolt | 5 | 6 | M8x20 mm | 25 N·m | 18 lb ft
Transmission Speed Sensor Bolt | 75 | 2 | M6x17 mm | 5.4 N·m | 48 lb in
Transmission Wiring Harness Bolt | 77 | 1 | M6x17 mm | 5.4 N·m | 48 lb in