For 1990-2009 cars

### Removal Procedure

1. Lower the molded headlining. Refer to Headlining Trim Panel Replacement.
2. Loosen the wing protective paneling inner.

2.1. | Remove the 2 bolts (1).

2.2. | Remove the 8 body-bound rivets (arrows).

Note: For better guidance with the installation, the water drain hose is to be provided with a cord.

3. Remove the water drain hose front.

3.1. | Remove the water drain hose from sunroof.

3.2. | Remove the water drain hose from the A-pillar bottom.

### Installation Procedure

1. Install the water drain hose front.

1.1. | Connect the water drain hose with cord.

1.2. | Draw in water drain hose in A-column carefully with the help of the cord.

1.3. | Remove the cord and install the water drain hose to the sunroof.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the wing protective paneling inner.

Install the 8 body-bound rivets.

Tighten
Tighten the 2 wheelhouse liner bolts to 2.5 N·m (22 lb in).

3. Install the molded headlining. Refer to Headlining Trim Panel Replacement.