For 1990-2009 cars

Connector 1: | X100 Transmission Harness to Automatic Transmission Harness (MNF)
Connector 2: | X101 Body Harness to Left Front Wheel Speed Sensor Harness
Connector 3: | X102 Forward Lamp Harness to Right Front Wheel Speed Sensor Harness
Connector 4: | X103 Forward Lamp Harness to Left Headlamp Harness
Connector 5: | X104 Forward Lamp Harness to Right Headlamp Harness
Connector 6: | X105 Forward Lamp Harness to Right Front Wheel Speed Sensor Harness
Connector 7: | X106 Power Steering Harness to Body Harness
Connector 8: | X107 Body Harness to Forward Lamp Harness
Connector 9: | X108 Body Harness to Engine and Transmission Harness
Connector 10: | X109 Engine Harness to Engine and Transmission Harness
Connector 11: | X110 Engine and Transmission Harness to Engine Control Module Harness
Connector 12: | X111 Cooling Fan Harness to Forward Lamp Harness
Connector 13: | X112 Forward Lamp Harness to Fog Lamp Harness
Connector 14: | X113 Transmission Harness to Engine and Transmission Harness (MNF)
Connector 15: | X114 Brake Booster Vacuum Pump Motor Harness to Body Harness
Connector 16: | X200 Instrument Panel Harness to Body Harness
Connector 17: | X201 Instrument Panel Harness to HVAC Harness
Connector 18: | X203 Instrument Panel Harness to Body Harness
Connector 19: | X204 Instrument Panel Harness to Transmission Harness (MNF)
Connector 20: | X250 Instrument Panel Harness to HVAC Auxiliary Harness
Connector 21: | X302 Radio Auxiliary Harness to Instrument Panel Harness
Connector 22: | X303 Dome Lamp Harness to Body Harness (- C3U)
Connector 23: | X304 Body Harness to Driver Seat Harness
Connector 24: | X305 Body Harness to Passenger Seat Harness
Connector 25: | X306 Transmission Harness to Automatic Transmission Shift Lock Control Jumper Harness (MNF)
Connector 26: | X307 Body harness to Sunroof Harness (C3U)
Connector 27: | X308 Body harness to Sunroof Harness (C3U)
Connector 28: | X309 Body Harness to Instrument Panel Harness
Connector 29: | X400 Fuel Tank Harness to Body Harness
Connector 30: | X401 Liftgate Extension Harness to Rear Body Harness
Connector 31: | X402 Rear Facia Harness to Body Rear Harness
Connector 32: | X403 Rear Axle ABS Harness to Body Harness
Connector 33: | X500 Body Harness to Driver Door Harness
Connector 34: | X600 Body Harness to Passenger Door Harness
Connector 35: | X700 Body Harness to Left Rear Door Harness (5 Door)
Connector 36: | X800 Body Harness to Right Rear Door Harness (5 Door)
Connector 37: | X901 Liftgate Extension Harness to Liftgate Harness

### X100 Transmission Harness to Automatic Transmission Harness (MNF)

#### Connector Part Information

- OEM:2-967564-1
- Service: Service by Harness - See Part Catalog
- Description: 16-Way F Sealed (GY)

#### Connector Part Information

- OEM: 2-968677-1
- Service: Service by Harness - See Part Catalog
- Description: 16-Way M Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X100 Transmission Harness to Automatic Transmission Harness (MNF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BK/GN | 1525 | Shift Solenoid Supply Voltage 1 | 1 | 0.5 WH | 1525 | Shift Solenoid Supply Voltage 1
2 | 0.5 BK/WH | 1527 | Shift Solenoid Supply Voltage 3 | 2 | 0.5 RD | 1527 | Shift Solenoid Supply Voltage 3
3 | 0.5 WH/GN | 1530 | Transmission Mainline Pressure Solenoid Control | 3 | 0.5 OG | 1530 | Transmission Mainline Pressure Solenoid Control
4 | 0.5 BK/BU | 585 | Transmission Oil Temperature Sensor Signal | 4 | 0.5 OG | 585 | Transmission Oil Temperature Sensor Signal
5 | 0.5 YE/RD | 1230 | Transmission Speed Sensor Signal | 5 | 0.5 YE/BK | 1230 | Transmission Speed Sensor Signal
6 | 0.5 YE/VT | 400 | Vehicle Speed Sensor Signal | 6 | 0.5 YE | 400 | Vehicle Speed Sensor Signal
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used
9 | 0.5 BK/VT | 1526 | Shift Solenoid Supply Voltage 2 | 9 | 0.5 BK | 1526 | Shift Solenoid Supply Voltage 2
10 | 0.5 WH/BK | 1994 | Shift Solenoid Control 4 | 10 | 0.5 YE | 1994 | Shift Solenoid Control 4
11 | 0.5 BU/WH | 5503 | Low Reference | 11 | 0.5 GN | 5503 | Low Reference
12 | 0.5 BN/BK | 586 | Low Reference | 12 | 0.5 OG | 586 | Low Reference
13 | 0.5 YE/BK | 1231 | Low Reference | 13 | 0.5 GN | 1231 | Low Reference
14 | 0.5 YE/BN | 401 | Low Reference | 14 | 0.5 GY | 401 | Low Reference
15 | 0.5 BN/GN | 2879 | Low Reference | 15 | 0.5 TN | 2879 | Low Reference
16 | -- | -- | Not Used | 16 | -- | -- | Not Used

### X101 Body Harness to Left Front Wheel Speed Sensor Harness

#### Connector Part Information

- OEM: 1452680-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 288041470838
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M Superseal 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X101 Body Harness to Left Front Wheel Speed Sensor Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/WH | 830 | Wheel Speed Sensor Signal Left Front | 1 | 0.5 BU/WH | 830 | Wheel Speed Sensor Signal Left Front
2 | 0.5 BN/WH | 873 | Low Reference | 2 | 0.5 BN/WH | 873 | Low Reference

### X102 Forward Lamp Harness to Right Front Wheel Speed Sensor Harness

#### Connector Part Information

- OEM: 1452680-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 288041470838
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M Superseal 1.5 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X102 Forward Lamp Harness to Right Front Wheel Speed Sensor Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front | 1 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front
2 | 0.5 BN/RD | 833 | Low Reference | 2 | 0.5 BN/RD | 833 | Low Reference

### X103 Forward Lamp Harness to Left Headlamp Harness

#### Connector Part Information

- OEM: 1-0967189-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way F Junior Power Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 1-962352-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X103 Forward Lamp Harness to Left Headlamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.5 BN | 1150 | Ground | 1 | BK | 1150 | Ground
BK | 1150 | Ground
2 | 1 WH | 711 | Left Headlamp High Beam Supply Voltage | 2 | BK | 711 | Left Headlamp High Beam Supply Voltage
3 | 1 YE | 712 | Left Headlamp Low Beam Supply Voltage | 3 | BK | 712 | Left Headlamp Low Beam Supply Voltage
4 | 0.5 GY/BK | 709 | Left Park Lamp Supply Voltage | 4 | BK | 709 | Left Park Lamp Supply Voltage
5 | 0.5 BK/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage | 5 | BK | 1314 | Left Front Turn Signal Lamp Supply Voltage
6-8 | -- | -- | Not Used | 6-8 | -- | -- | Not Used
9 | 1.5 BN | 1150 | Ground | 9 | BK | 1150 | Ground
10 | 1.5 BN | 1150 | Ground | 10 | BK | 1150 | Ground

### X104 Forward Lamp Harness to Right Headlamp Harness

#### Connector Part Information

- OEM: 1-0967189-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way F Junior Power Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 1-9623521-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X104 Forward Lamp Harness to Right Headlamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.5 BN | 1050 | Ground | 1 | BK | 1050 | Ground
BK | 1050 | Ground
2 | 1 WH | 311 | Right Headlamp High Beam Supply Voltage | 2 | BK | 311 | Right Headlamp High Beam Supply Voltage
3 | 1 YE | 312 | Right Headlamp Low Beam Supply Voltage | 3 | BK | 312 | Right Headlamp Low Beam Supply Voltage
4 | 0.5 GY/BK | 309 | Right Park Lamp Supply Voltage | 4 | BK | 309 | Right Park Lamp Supply Voltage
5 | 0.5 BK/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage | 5 | BK | 1315 | Right Front Turn Signal Lamp Supply Voltage
6-8 | -- | -- | Not Used | 6-8 | -- | -- | Not Used
9 | 1.5 BN | 1050 | Ground | 9 | BK | 1050 | Ground
10 | 1.5 BN | 10150 | Ground | 10 | BK | 1050 | Ground

### X105 Forward Lamp Harness to Right Front Wheel Speed Sensor Harness

#### Connector Part Information

- OEM: 1452680-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series Sealed (BK)

#### Connector Part Information

- OEM: 288041470838
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M Superseal 1.5 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X105 Forward Lamp Harness to Right Front Wheel Speed Sensor Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front | 1 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front
2 | 0.5 BN/RD | 833 | Low Reference | 2 | 0.5 BN/RD | 833 | Low Reference

### X106 Power Steering Harness to Body Harness

#### Connector Part Information

- OEM: ZFW5-22
- Service: Service by Harness - See Part Catalog
- Description: 5-Way F Sealed (BK)

#### Connector Part Information

- OEM: 1928404590
- Service: Service by Harness - See Part Catalog
- Description: 5-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X106 Power Steering Harness to Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BK | 639 | Run/Crank Ignition 1 Voltage | 1 | 0.5 BK | 639 | Run/Crank Ignition 1 Voltage
2 | 0.75 GN | 2500 | High Speed GMLAN Serial Data (+) (NS2/NR1) | 2 | 0.75 GN | 2500 | High Speed GMLAN Serial Data (+)
3 | 0.75 WH | 2501 | High Speed GMLAN Serial Data (-) (NS2/NR1) | 3 | 0.75 WH | 2501 | High Speed GMLAN Serial Data (-)
4 | 0.5 GN/WH | 377 | Serial Data (- NS2/NR1) | 4 | 0.5 GN/WH | 377 | Serial Data
5 | 0.5 BU/WH | 225 | Generator Turn On Signal (- NS2/NR1) | 5 | 0.5 BU/WH | 225 | Generator Turn On Signal

### X107 Body Harness to Forward Lamp Harness

#### Connector Part Information

- OEM: 60432101
- Service: Service by Harness - See Part Catalog
- Description: 48-Way F 1.5, 5.8 Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 60531801
- Service: 93186683
- Description: 48-Way M 1.5, 5.8 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X107 Body Harness to Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-6 | -- | -- | Not Used | 1-6 | -- | -- | Not Used
7 | 0.5 YE/GY | 6776 | Middle Front Impact Sensing Module 2 Supply Voltage | 7 | 0.5 YE/GY | 6776 | Middle Front Impact Sensing Module 2 Supply Voltage
8 | 0.5 GN/WH | 6777 | Middle Front Impact Sensing Module 2 Signal | 8 | 0.5 GN/WH | 6777 | Middle Front Impact Sensing Module 2 Signal
9 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front | 9 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front
10 | 0.5 BN/RD | 833 | Low Reference | 10 | 0.5 BN/RD | 833 | Low Reference
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | 0.5 BK/WH | 6168 | Middle Front Impact Sensing Module Supply Voltage | 12 | 0.5 BK/WH | 6168 | Middle Front Impact Sensing Module Supply Voltage
13 | 0.5 OG/BK | 6169 | Middle Front Impact Sensing Module Signal | 13 | 0.5 OG/BK | 6169 | Middle Front Impact Sensing Module Signal
14 | 0.5 BK/GN | 1415 | Right Front Turn Signal Switch Signal | 14 | 0.5 BK/GN | 1415 | Right Front Turn Signal Switch Signal
15 | 0.5 BK/WH | 1414 | Left Front Turn Signal Switch Signal | 15 | 0.5 BK/WH | 1414 | Left Front Turn Signal Switch Signal
16-32 | -- | -- | Not Used | 16-32 | -- | -- | Not Used
33 | 2.5 RD | 342 | Battery Positive Voltage | 33 | 2.5 RD | 342 | Battery Positive Voltage
34-48 | -- | -- | Not Used | 34-48 | -- | -- | Not Used

### X108 Body Harness to Engine and Transmission Harness

#### Connector Part Information

- OEM: 1-967189-1
- Service: 88988927
- Description: 10-Way F Junior Power Timer Series (BK)

#### Connector Part Information

- OEM: 1452546-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way M Junior Power Timer Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X108 Body Harness to Engine and Transmission Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BN/YE | 251 | Low Reference | 1 | 0.5 BU/TN | 251 | Low Reference
2 | 0.5 BN | 30 | Fuel Level Sensor Signal | 2 | 0.5 BU | 30 | Fuel Level Sensor Signal
3 | 1 BU | 5372 | Ignition Voltage | 3 | 1 RD/BK | 5291 | Ignition Voltage
4 | 1 GN | 2350 | EVAP Canister Vent Solenoid Control | 4 | 1 TN | 2350 | EVAP Canister Vent Solenoid Control
5 | 0.5 BN/YE | 998 | MIL Control | 5 | 0.5 BK | 998 | MIL Control
6 | 0.5 BK | 1039 | ECM Starter Control | 6 | 0.5 BU/BK | 1039 | ECM Starter Control (M25)
7 | 0.5 VT | 1935 | CPP Starter Control | 7 | 0.5 BU/BK | 1935 | CPP Starter Control (M25)
8-10 | -- | -- | Not Used | 8-10 | -- | -- | Not Used

### X109 Engine Harness to Engine and Transmission Harness

#### Connector Part Information

- OEM: ZFW6
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK w/RD Lock)

#### Connector Part Information

- OEM: ZMW6
- Service: Service by Harness - See Part Catalog
- Description: 6-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X109 Engine Harness to Engine and Transmission Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/WH | 225 | Generator Turn On Signal | 1 | 0.5 BU/WH | 225 | Generator Turn On Signal
2 | 2.5 BK/RD | 6 | Starter Solenoid Crank Voltage | 2 | 2.5 BK/RD | 6 | Starter Solenoid Crank Voltage
3-6 | -- | -- | Not Used | 3-6 | -- | -- | Not Used

### X110 Engine and Transmission Harness to Engine Control Module Harness

#### Connector Part Information

- OEM: ZFW11
- Service: Service by Harness - See Part Catalog
- Description: 11-Way F Sealed (BK)

#### Connector Part Information

- OEM: ZMW11
- Service: Service by Harness - See Part Catalog
- Description: 11-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X110 Engine and Transmission Harness to Engine Control Module Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | 1 BN/BK | 260 | Fuel Injection Control | 3 | 1 RD/BU | 260 | Fuel Injection Control
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 1.5 BK | 39 | Run/Crank Ignition 1 Voltage | 5 | 1.5 BK | 39 | Run/Crank Ignition 1 Voltage
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | 2.5 OG/BK | 5291 | Ignition Voltage | 8 | 2.5 OG/BK | 5291 | Ignition Voltage
9-11 | -- | -- | Not Used | 9-11 | -- | -- | Not Used

### X111 Cooling Fan Harness to Forward Lamp Harness

#### Connector Part Information

- OEM: ZFW13
- Service: See Catalog
- Description: 13-Way F Sealed (BK)

#### Connector Part Information

- OEM: 15439852
- Service: 93186717
- Description: 13-Way M 1.6, 2.8, 6.3 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X111 Cooling Fan Harness to Forward Lamp Harness (C60)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.5 BK/WH | 59 | A/C Compressor Clutch Supply Voltage (C60) | 1 | 1.5 BK/WH | 59 | A/C Compressor Clutch Supply Voltage (C60)
2 | 1.5 BN/RD | 1250 | Ground | 2 | 1.5 BN | 1250 | Ground
3 | 6 RD/WH | 532 | Cooling Fan Motor Supply Voltage 2 (MNF) | 3 | 6 RD/WH | 532 | Cooling Fan Motor Supply Voltage 2 (MNF)
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.5 BK/WH | 2700 | 5 Volt Reference 1 (C60) | 5 | 0.5 BK/WH | 2700 | 5 Volt Reference 1 (C60)
6 | 0.5 GN | 380 | A/C Refrigerant Pressure Sensor Signal (C60) | 6 | 0.5 GN | 380 | A/C Refrigerant Pressure Sensor Signal (C60)
7 | 0.5 BN/BK | 5514 | Low Reference (C60) | 7 | 0.5 BN/BK | 5514 | Low Reference (C60)
8-11 | -- | -- | Not Used | 8-9 | -- | -- | Not Used
12 | 4 RD/WH | 532 | Cooling Fan Motor Supply Voltage 2 (M25) | 12 | 4 RD/WH | 532 | Cooling Fan Motor Supply Voltage 2 (M25)
6 BN/GN | 504 | Low Reference (MNF) | 6 RD/WH | 504 | Low Reference (MNF)
13 | 4 RD/YE | 409 | Cooling Fan Motor Supply Voltage 1 | 13 | 4 RD/YE | 409 | Cooling Fan Motor Supply Voltage 1

### X112 Forward Lamp Harness to Fog Lamp Harness

#### Connector Part Information

- OEM: 15326849
- Service: 88986260
- Description: 12-Way F GT 150 280 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15326854
- Service: See Catalog
- Description: 12-Way M GT 150 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X112 Forward Lamp Harness to Fog Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 1.5 BN | 1150 | Ground (T96) | A | 1.5 BN | 1150 | Ground (T96)
B | 1.5 BN/GY | 5061 | Left Front Fog Lamp Supply Voltage (T96) | B | 1.5 BN/GY | 5061 | Left Front Fog Lamp Supply Voltage (T96)
C | 1.5 BN | 1050 | Ground (T96) | C | 1.5 BN | 1050 | Ground (T96)
D | 1.5 BN/GN | 5062 | Right Front Fog Lamp Supply Voltage (T96) | D | 1.5 BN/GN | 5062 | Right Front Fog Lamp Supply Voltage (T96)
E | 0.5 BU | 636 | Outside Ambient Air Temperature Sensor Signal | E | 0.5 BU | 636 | Outside Ambient Air Temperature Sensor Signal
F | 0.5 BU/BN | 61 | Low Reference | F | 0.5 BU/BN | 61 | Low Reference
G | 0.5 BN | 1150 | Ground | G | 0.5 BN | 1150 | Ground
H | 0.5 BK/WH | 1414 | Left Front Turn Signal Switch Signal | H | 0.5 BK/WH | 1414 | Left Front Turn Signal Switch Signal
J | 0.5 BN | 1050 | Ground | J | 0.5 BN | 1050 | Ground
K | 0.5 BK/GN | 1415 | Right Front Turn Signal Switch Signal | K | 0.5 BK/GN | 1415 | Right Front Turn Signal Switch Signal
L | 0.5 BU | 636 | Outside Ambient Air Temperature Sensor Signal | L | 0.5 BU | 636 | Outside Ambient Air Temperature Sensor Signal
M | 0.5 BU/BN | 61 | Low Reference | M | 0.5 BU/BN | 61 | Low Reference

### X113 Transmission Harness to Engine and Transmission Harness (MNF)

#### Connector Part Information

- OEM: 1-0967189-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way F Sealed (BK)

#### Connector Part Information

- OEM: 12186711
- Service: Service by Harness - See Part Catalog
- Description: 10-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X113 Transmission Harness to Engine and Transmission Harness (MNF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.5 BK | 539 | Run/Crank Ignition 1 Voltage | 1 | 1.5 BK | 539 | Run/Crank Ignition 1 Voltage
2 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+) | 2 | 0.5 BU | 2500 | High Speed GMLAN Serial Data (+)
3 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-) | 3 | 0.5 GN | 2501 | High Speed GMLAN Serial Data (-)
4 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+) | 4 | 0.5 BU | 2500 | High Speed GMLAN Serial Data (+)
5 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-) | 5 | 0.5 GN | 2501 | High Speed GMLAN Serial Data (-)
6 | 0.75 RD | 3740 | Battery Positive Voltage | 6 | 0.75 RD | 3740 | Battery Positive Voltage
7 | 0.5 WH | 771 | Transmission Position Switch Bit 1 Signal | 7 | 0.5 WH | 771 | Transmission Position Switch Bit 1 Signal
8 | 0.5 GN | 772 | Transmission Position Switch Bit 2 Signal | 8 | 0.5 GN/WH | 772 | Transmission Position Switch Bit 2 Signal
9 | 0.5 GY | 773 | Transmission Position Switch Bit 3 Signal | 9 | 0.5 GY | 773 | Transmission Position Switch Bit 3 Signal
10 | 0.5 WH/YE | 1371 | Transmission Position Switch Bit 4 Signal | 10 | 0.5 WH/YE | 1371 | Transmission Position Switch Bit 4 Signal

### X114 Brake Booster Vacuum Pump Motor Harness to Body Harness

#### Connector Part Information

- OEM: 1928403428
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X114 Brake Booster Vacuum Pump Motor Harness to Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 2.5 BN | 1350 | Ground | A | 2.5 BN | 1350 | Ground
B | 2.5 BK | 7448 | Brake Booster Pump Supply Voltage | B | 2.5 BK | 7448 | Brake Booster Pump Supply Voltage

### X200 Instrument Panel Harness to Body Harness

#### Connector Part Information

- OEM: 1355713-1
- Service: Service by Harness - See Part Catalog
- Description: 102-Way F 1.5, 2.5, 9.5 Series (BK)

#### Connector Part Information

- OEM: 1452764-1
- Service: Service by Harness - See Part Catalog
- Description: 102-Way M 1.5, 2.5, 9.5 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X200 Instrument Panel Harness to Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BN/RD | 1271 | Low Reference | 1 | 0.5 BN/RD | 1271 | Low Reference
2 | 0.5 BK/RD | 1164 | 5 Volt Reference 1 | 2 | 0.5 BK/RD | 1164 | 5 Volt Reference 1
3 | 0.5 WH/YE | 1161 | Accelerator Pedal Position Signal 1 | 3 | 0.5 WH/YE | 1161 | Accelerator Pedal Position Signal 1
4 | 0.5 BN/WH | 1272 | Low Reference | 4 | 0.5 BN/WH | 1272 | Low Reference
5 | 0.5 BK/YE | 1274 | 5 Volt Reference 2 | 5 | 0.5 BK/YE | 1274 | 5 Volt Reference 2
6 | 0.5 WH/GN | 1162 | Accelerator Pedal Position Signal 2 | 6 | 0.5 WH/GN | 1162 | Accelerator Pedal Position Signal 2
7 | 0.5 RD | 1542 | Battery Positive Voltage (C60) | 7 | 0.5 RD | 1542 | Battery Positive Voltage
8 | 0.5 OG/WH | 5018 | Occupant Sensor Serial Data | 8 | 0.5 OG/WH | 5018 | Occupant Sensor Serial Data
9-11 | -- | -- | Not Used | 9-11 | -- | -- | Not Used
12 | 0.75 BK | 839 | Run/Crank Ignition 1 Voltage | 12 | 0.75 BK | 839 | Run/Crank Ignition 1 Voltage
13 | 0.5 BK/YE | 1733 | Inadvertant Power Courtesy Lamp | 13 | 0.5 BK/YE | 1733 | Inadvertant Power Courtesy Lamp
14-15 | -- | -- | Not Used | 14-15 | -- | -- | Not Used
16 | 0.5 GY/YE | 1382 | LED Dimming Signal | 16 | 0.5 GY/YE | 1382 | LED Dimming Signal
17 | 0.75 RD | 1742 | Battery Positive Voltage | 17 | 0.75 RD | 1742 | Battery Positive Voltage
18 | 0.5 VT | 1935 | CPP Starter Control | 18 | 0.5 VT | 1935 | CPP Starter Control
19 | 0.5 BU/BN | 1903 | ABS Wheel Speed Sensor Signal Left Front | 19 | 0.5 BU/BN | 1903 | ABS Wheel Speed Sensor Signal Left Front
20 | 0.5 BK | 1039 | ECM Starter Control | 20 | 0.5 BK | 1039 | ECM Starter Control
21 | 0.5 BK/BN | 848 | Brake Switch Signal | 21 | 0.5 BK/BN | 848 | Brake Switch Signal
22 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal | 22 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal
23 | 0.5 RD/BU | 5293 | Ignition Voltage | 23 | 0.5 RD/BU | 5293 | Ignition Voltage
24 | 0.5 RD | 302 | Battery Positive Voltage | 24 | 0.5 RD | 302 | Battery Positive Voltage
25 | 0.5 GN/WH | 377 | Serial Data | 25 | 0.5 GN/WH | 377 | Serial Data
26 | 0.75 RD | 1442 | Battery Positive Voltage | 26 | 0.75 RD | 1442 | Battery Positive Voltage
27 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-) | 27 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-)
28 | 0.75 BU | 201 | Left Front Speaker (+) | 28 | 0.75 BU | 201 | Left Front Speaker (+)
29 | 0.75 YE | 200 | Right Front Speaker (+) | 29 | 0.75 YE | 200 | Right Front Speaker (+)
30 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-) | 30 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-)
31 | 0.75 GN | 199 | Left Rear Speaker (+) | 31 | 0.75 GN | 199 | Left Rear Speaker (+)
32 | 0.75 BN/GN | 116 | Left Rear Speaker Signal (-) | 32 | 0.75 BN/GN | 116 | Left Rear Speaker Signal (-)
33-36 | -- | -- | Not Used | 33-36 | -- | -- | Not Used
37 | 0.5 BK | 1039 | Run/Crank Ignition 1 Voltage | 37 | 0.5 BK | 1039 | Run/Crank Ignition 1 Voltage
38 | 0.5 GY | 379 | Cruise Control Clutch Pedal Position Switch Signal | 38 | 0.5 GY | 379 | Cruise Control Clutch Pedal Position Switch Signal
39-40 | -- | -- | Not Used | 39-40 | -- | -- | Not Used
41 | 0.5 VT/BN | 5968 | Driver Door Lock Status Indicator Signal | 41 | 0.5 VT/BN | 5968 | Driver Door Lock Status Indicator Signal
42 | -- | -- | Not Used | 42 | -- | -- | Not Used
43 | 0.75 BK | 3 | Run/Crank Ignition 1 Voltage | 43 | 0.75 BK | 3 | Run/Crank Ignition 1 Voltage
44 | 0.5 BK | 239 | Run/Crank Ignition 1 Voltage | 44 | 0.5 BK | 239 | Run/Crank Ignition 1 Voltage
45 | 0.75 RD | 3140 | Battery Positive Voltage | 45 | 0.75 RD | 3140 | Battery Positive Voltage
46 | 0.75 RD | 1540 | Battery Positive Voltage | 46 | 0.75 RD | 1540 | Battery Positive Voltage
47 | 0.5 BN/RD | 1134 | Park Brake Switch Signal | 47 | 0.5 BN/RD | 1134 | Park Brake Switch Signal
48 | 0.5 BN/GY | 1462 | Driver Heated Seat Switch Control (KA1) | 48 | 0.5 BN/GY | 1462 | Driver Heated Seat Switch Control (KA1)
49 | 0.5 BK/YE | 1505 | Front Passenger Heated Seat Switch Control (KA1) | 49 | 0.5 BK/YE | 1505 | Front Passenger Heated Seat Switch Control (KA1)
50 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data | 50 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
51 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data | 51 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
52 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-) | 52 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
53 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+) | 53 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
54 | -- | -- | Not Used | 54 | -- | -- | Not Used
55 | 0.5 BN/WH | 28 | Horn Relay Control | 55 | 0.5 BN/WH | 28 | Horn Relay Control
56-57 | -- | -- | Not Used | 56-57 | -- | -- | Not Used
58 | 0.5 GN/WH | 2514 | Keypad Signal | 58 | 0.5 GN/WH | 2514 | Keypad Signal
59 | 0.5 OG/BK | 2518 | 10-Volt Reference | 59 | 0.5 OG/BK | 2518 | 10-Volt Reference
60 | 0.5 YE/BK | 2516 | Keypad Green LED | 60 | 0.5 YE/BK | 2516 | Keypad Green LED
61 | 0.5 BN/WH | 2517 | Keypad Red LED | 61 | 0.5 BN/WH | 2517 | Keypad Red LED
62 | 0.5 WH | 194 | Door Unlock Control | 62 | 0.5 WH | 194 | Door Unlock Control
63-64 | -- | -- | Not Used | 63-64 | -- | -- | Not Used
65 | 0.5 BN/YE | 998 | MIL Control | 65 | 0.5 BN/YE | 998 | MIL Control
66 | 0.35 BK | 5193 | Low Reference | 66 | 0.35 BK | 5193 | Low Reference
67-76 | -- | -- | Not Used | 67-76 | -- | -- | Not Used
77 | 0.35 BU/RD | 5191 | Cellular Telephone Microphone Signal | 77 | 0.35 BU/RD | 5191 | Cellular Telephone Microphone Signal
78-86 | -- | -- | Not Used | 78-86 | -- | -- | Not Used
87 | 0.75 BN/WH | 115 | Right Rear Speaker Signal (-) | 87 | 0.75 BN/WH | 115 | Right Rear Speaker Signal (-)
88 | 0.75 WH | 46 | Right Rear Speaker (+) | 88 | 0.75 WH | 46 | Right Rear Speaker (+)
89 | -- | -- | Not Used | 89 | -- | -- | Not Used
90 | 4 BK | 1241 | Run Ignition 3 Voltage | 90 | 4 BK | 1241 | Run Ignition 3 Voltage
91 | 1.5 RD | 502 | Battery Positive Voltage | 91 | 1.5 RD | 502 | Battery Positive Voltage
92 | -- | -- | Not Used | 92 | -- | -- | Not Used
93 | 2.5 RD | 3040 | Battery Positive Voltage | 93 | 2.5 RD | 3040 | Battery Positive Voltage
94-102 | -- | -- | Not Used | 94-102 | -- | -- | Not Used

### X201 Instrument Panel Harness to HVAC Harness

#### Connector Part Information

- OEM: ZF14-6
- Service: Service by Harness - See Part Catalog
- Description: 14-Way F (BK)

#### Connector Part Information

- OEM: ZM14-6
- Service: Service by Harness - See Part Catalog
- Description: 14-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X201 Instrument Panel Harness to HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BN | 1650 | Ground | 1 | 1 YE/BK | 1650 | Ground
2 | 0.5 GY/YE | 1382 | LED Dimming Signal | 2 | 0.5 GN | 1382 | LED Dimming Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | 0.5 BK/WH | 292 | Rear Defog Switch Signal | 4 | 0.5 BU | 292 | Rear Defog Switch Signal
5 | 0.5 BN/WH | 193 | Rear Defog Relay Control | 5 | 0.5 BN/WH | 193 | Rear Defog Relay Control
6 | 0.5 BK/VT | 66 | A/C Request Signal (C60) | 6 | 0.5 BK/WH | 66 | A/C Request Signal (C60)
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | 0.5 RD | 1542 | Battery Positive Voltage (C60) | 8 | 0.5 OG | 1542 | Battery Positive Voltage (C60)
9 | 0.75 BK | 839 | Run/Crank Ignition 1 Voltage | 9 | 0.75 YE/GN | 839 | Run/Crank Ignition 1 Voltage
10-12 | -- | -- | Not Used | 10-12 | -- | -- | Not Used
13 | 4 BK | 1241 | Run Ignition 3 Voltage | 13 | 4 RD | 1241 | Run Ignition 3 Voltage
14 | 4 BN | 1850 | Ground | 14 | 4 BK | 1850 | Ground

### X203 Instrument Panel Harness to Body Harness

#### Connector Part Information

- OEM: 355726-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (WH)

#### Connector Part Information

- OEM: 1355729-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X203 Instrument Panel Harness to Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 COAX | 6794 | GSM Antenna Signal | 1 | 0.35 COAX | 6794 | GSM Antenna Signal
2 | 0.35 COAX | 5174 | Antenna Navigation Signal | 2 | 0.35 COAX | 5174 | Antenna Navigation Signal

### X204 Instrument Panel Harness to Transmission Harness (MNF)

#### Connector Part Information

- OEM: 15426890
- Service: Service by Harness - See Part Catalog
- Description: 12-Way F 1.2 Series (BK)

#### Connector Part Information

- OEM: 15426894
- Service: Service by Harness - See Part Catalog
- Description: 12-Way M 1.2 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X204 Instrument Panel Harness to Transmission Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BN | 2150 | Ground | 1 | 1 BN | 2150 | Ground (MNF)
2 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal | 2 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal (MNF)
3 | 0.5 GY/YE | 1382 | LED Dimming Signal | 3 | 0.5 GY/YE | 1382 | LED Dimming Signal (MNF)
4-12 | -- | -- | Not Used | 4-12 | -- | -- | Not Used

### X250 Instrument Panel Harness to HVAC Auxiliary Harness

#### Connector Part Information

- OEM: 968571-1
- Service: Service by Harness - See Part Catalog
- Description: 9-Way F 64 MQS Series, (GY)

#### Connector Part Information

- Harness: Option Not Available
- OEM: Option Not Available
- Service: Option Not Available
- Description: Option Not Available

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminated Lead: Option Not Available

#### X250 Instrument Panel Harness to HVAC Auxiliary Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 839 | Run/Crank Ignition 1 Voltage | 1 | -- | -- | Option Not Available
2 | -- | -- | Not Used | 2 | -- | -- | Option Not Available
3 | GN | 5060 | Low Speed GMLAN Serial Data | 3 | -- | -- | Option Not Available
4-6 | -- | -- | Not Used | 4-6 | -- | -- | Option Not Available
7 | BN | 1850 | Ground | 7 | -- | -- | Option Not Available
8-9 | -- | -- | Not Used | 8-9 | -- | -- | Option Not Available

### X302 Radio Auxiliary Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: 1452142-1
- Service: 93186706
- Description: 3-Way F (BK)

#### Connector Part Information

- OEM: 1-962342-1
- Service: Service by Harness - See Part Catalog
- Description: 3-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186706
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X302 Radio Auxiliary Harness to Instrument Panel Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 VT/RD | 5841 | Upfitter Provision | 1 | 0.35 VT/RD | 5841 | Right Auxiliary Audio Signal 2
2 | 0.35 VT/WH | 5839 | Upfitter Provision | 2 | 0.35 VT/WH | 5839 | Left Auxiliary Audio Signal 2
3 | 0.35 BK | 5842 | Upfitter Provision | 3 | 0.35 BK | 5842 | Auxiliary Audio Screen 2

### X303 Dome Lamp Harness to Body Harness (- C3U)

#### Connector Part Information

- OEM: F9-35
- Service: Service by Harness - See Part Catalog
- Description: 9-Way F MTS 0.64 Series (BK)

#### Connector Part Information

- OEM: 284803-1
- Service: Service by Harness - See Part Catalog
- Description: 9-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X303 Dome Lamp Harness to Body Harness (- C3U)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 FW | 157 | Interior Lamp Control | 1 | 0.5 GY | 157 | Interior Lamp Control
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | 0.5 FW | 1732 | Inadvertant Power Courtesy Lamp | 3 | 0.5 RD/BU | 1732 | Inadvertant Power Courtesy Lamp
4 | 0.5 FW | 1550 | Ground | 4 | 0.5 BN | 1550 | Ground
5-9 | -- | -- | Not Used | 5-9 | -- | -- | Not Used

### X304 Body Harness to Driver Seat Harness

#### Connector Part Information

- OEM: ZF 16-11
- Service: Service by Harness - See Part Catalog
- Description: 16-Way F (BK)

#### Connector Part Information

- OEM: ZUH 291
- Description: 16-Way M Connector Housing (BK)

#### Connector Part Information

- OEM: ZM2-20
- Service: Service by Component Assembly - See Part Catalog
- Description: 2-Way M (YE)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM4-13
- Service: Service by Component Assembly - See Part Catalog
- Description: 4-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM2-19
- Service: Service by Component Assembly - See Part Catalog
- Description: 2-Way M (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM4-12
- Service: Service by Component Assembly - See Part Catalog
- Description: 4-Way M (GN)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### X304 Body Harness to Driver Seat Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 OG/BU | 2137 | Left Front Side Impact Module High Control | 1 | 0.5 BU | 2137 | Left Front Side Impact Module High Control
2 | 0.5 BU | 2138 | Left Front Side Impact Module Low Control | 2 | 0.5 BN | 2138 | Left Front Side Impact Module Low Control
3-6 | -- | -- | Not Used | 1-4 | -- | -- | Not Available
7 | 0.5 BN/GY | 1462 | Heated Seat Switch Signal (KA1) | 1 | 0.5 BN/GY | 1462 | Heated Seat Switch Signal (KA1)
8 | 1.5 BK | 1041 | Run Ignition 3 Voltage (KA1) | 2 | 1.5 BK | 1041 | Run Ignition 3 Voltage (KA1)
9 | 1 BN | 2150 | Ground (KA1) | 3 | 1 BN | 2150 | Ground (KA1)
10 | -- | -- | Not Used (KA1) | 4 | -- | -- | Not Used (KA1)
11 | 0.5 BN/WH | 238 | Driver Seat Belt Switch Signal | 1 | 0.5 BK | 238 | Driver Seat Belt Switch Signal
12 | 0.5 VT/BK | 1363 | Low Reference | 2 | 0.5 BK | 1363 | Low Reference
13-14 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
15 | 0.5 OG/BN | 2118 | Driver Seat Belt Pretensioner High Control | 3 | 0.5 BU | 2118 | Driver Seat Belt Pretensioner High Control
16 | 0.5 BN | 2119 | Driver Seat Belt Pretensioner Low Control | 4 | 0.5 BN | 2119 | Driver Seat Belt Pretensioner Low Control

### X305 Body Harness to Passenger Seat Harness

#### Connector Part Information

- OEM: ZFW16-11
- Service: Service by Harness - See Part Catalog
- Description: 16-Way F (BK)

#### Connector Part Information

- OEM: ZUH 291
- Description: 16-Way M Connector Housing (BK)

#### Connector Part Information

- OEM: ZM2-20
- Service: Service by Component Assembly - See Part Catalog
- Description: 2-Way M (YE)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM4-14
- Service: Service by Component Assembly - See Part Catalog
- Description: 4-Way M (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM4-13
- Service: Service by Component Assembly - See Part Catalog
- Description: 4-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM2-19
- Service: Service by Component Assembly - See Part Catalog
- Description: 2-Way M (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### Connector Part Information

- OEM: ZM4-12
- Service: Service by Component Assembly - See Part Catalog
- Description: 4-Way M (GN)

#### Terminal Part Information

- Terminal/Tray: Service by Component Assembly - See Part Catalog
- Release Tool/Test Probe: N/A

#### X305 Body Harness to Passenger Seat Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 OG/BK | 2103 | Right Side Impact Module High Control | 1 | 0.5 BU | 2103 | Right Side Impact Module High Control
2 | 0.5 BK/WH | 2104 | Right Side Impact Module Low Control | 2 | 0.5 BN | 2104 | Right Side Impact Module Low Control
3-4 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
5 | 0.5 BU/YE | 5056 | Passenger Seat Position Switch Signal | 3 | 0.5 BK | 5056 | Passenger Seat Position Switch Signal
6 | 0.5 BU/BK | 1361 | Low Reference | 4 | 0.5 BN | 1361 | Low Reference
7 | 0.5 BK/YE | 1505 | Passenger Heated Seat Switch Signal (KA1) | 1 | 0.5 BN/GY | 1505 | Passenger Heated Seat Switch Signal (KA1)
8 | 1.5 BK | 1341 | Run Ignition 3 Voltage (KA1) | 2 | 1.5 BK | 1341 | Run Ignition 3 Voltage (KA1)
9 | 1 BN | 2150 | Ground (KA!) | 3 | 1 BN | 2150 | Ground (KA1)
10 | -- | -- | Not Used (KA1) | 4 | -- | -- | Not Used (KA1)
11 | 0.5 BU | 1362 | Passenger Seat Belt Switch Signal | 1 | 0.5 BK | 1362 | Passenger Seat Belt Switch Signal
12 | 0.5 BU/BK | 1361 | Passenger Seat Belt Switch Low Reference | 2 | 0.5 BK | 1361 | Passenger Seat Belt Switch Low Reference
13-14 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
15 | 0.5 OG/GY | 2116 | Passenger Seat Belt Pretensioner High Control | 3 | 0.5 BU | 2116 | Passenger Seat Belt Pretensioner High Control
16 | 0.5 BU | 2117 | Passenger Seat Belt Pretensioner Low Control | 4 | 0.5 BN | 2117 | Passenger Seat Belt Pretensioner Low Control

### X306 Transmission Harness to Automatic Transmission Shift Lock Control Jumper Harness (MNF)

#### Connector Part Information

- OEM: 928523-1
- Service: Service by Harness - See Part Catalog
- Description: 9-Way F (WH)

#### Connector Part Information

- OEM: M9-23
- Service: Service by Harness - See Part Catalog
- Description: 9-Way M (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X306 Transmission Harness to Automatic Transmission Shift Lock Control Jumper Harness (MNF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 GN | 1078 | Ignition Key/Shifter Interlock Solenoid Lock Signal | 1 | 0.5 GN | 1078 | Ignition Key/Shifter Interlock Solenoid Lock Signal
2-5 | -- | -- | Not Used | 2-5 | -- | -- | Not Used
6 | 0.5 BN | 2150 | Ground | 6 | 0.5 BN | 2150 | Ground
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal | 8 | 0.5 YE | 17 | Stop Lamp Switch Signal
9 | -- | -- | Not Used | 9 | -- | -- | Not Used

### X307 Body harness to Sunroof Harness (C3U)

#### Connector Part Information

- OEM: 365060-1
- Service: 93185233
- Description: 4-Way F Junior Timer Series, (WH)

#### Connector Part Information

- OEM: 365059-1
- Service: Service by Harness - See Part Catalog
- Description: 4-Way M (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93185233
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X307 Body harness to Sunroof Harness (C3U)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.5 BN | 1550 | Ground | 1 | 2.5 BK | 1550 | Ground
2 | 2.5 RD | 140 | Battery Positive Voltage | 2 | 2.5 RD | 140 | Battery Positive Voltage
3 | 2.5 BN | 1550 | Ground | 3 | 2.5 BK | 1550 | Ground
4 | 2.5 RD | 142 | Battery Positive Voltage | 4 | 2.5 RD | 142 | Battery Positive Voltage

### X308 Body harness to Sunroof Harness (C3U)

#### Connector Part Information

- OEM: 968571-1
- Service: 93180750
- Description: 9-Way F 64 MQS Series, (GY)

#### Connector Part Information

- OEM: 284803-1
- Service: Service by Harness - See Part Catalog
- Description: 9-Way M MQS Series, (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X308 Body harness to Sunroof Harness (C3U)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/WH | 110 | Sunroof Switch Close Signal | 1 | 0.5 OG | 110 | Sunroof Switch Close Signal
2 | 0.5 GN/WH | 129 | Sunroof Shade Switch Close Signal | 2 | 0.5 OG | 129 | Sunroof Shade Switch Close Signal
3 | 0.5 GY | 157 | Interior Lamp Control | 3 | 0.5 YE | 157 | Interior Lamp Control
4 | 0.5 RD/BU | 1732 | Inadvertant Power Courtesy Lamp | 5 | 0.5 GN | 1732 | Inadvertant Power Courtesy Lamp
5 | 0.5 BN | 1550 | Ground | 5 | 0.5 WH | 1550 | Ground
6 | 0.5 GY/YE | 1382 | LED Dimming Signal | 6 | 0.5 RD | 1382 | LED Dimming Signal
7 | 0.5 BK | 4 | Accessory Voltage | 7 | 0.5 BU | 4 | Accessory Voltage
8 | -- | -- | Not Used | 8 | 0.5 | GY | Not Used
9 | -- | -- | Not Used | 9 | -- | -- | Not Used

### X309 Body Harness to Instrument Panel Harness

#### Connector Part Information

- OEM: 1355728-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (GY)

#### Connector Part Information

- OEM: 1355727-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X309 Body Harness to Instrument Panel Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.35 BK | 5172 | Antenna Radio Signal | 2 | 0.35 BK | 5172 | Antenna Radio Signal

### X400 Fuel Tank Harness to Body Harness

#### Connector Part Information

- OEM: 15326849
- Service: Service by Harness - See Part Catalog
- Description: 12-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15336135
- Service: 15306125
- Description: 12-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X400 Fuel Tank Harness to Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 1.5 RD/BU | 120 | Fuel Pump Supply Voltage | A | 1.5 RD/BU | 120 | Fuel Pump Supply Voltage
B | 1.5 BN | 2350 | Ground | B | 1.5 BN | 2350 | Ground
C | 0.5 BN/YE | 251 | Low Reference | C | 0.5 BN/YE | 251 | Low Reference
D | 0.5 GN/BU | 30 | Fuel Level Sensor Signal | D | 0.5 GN/BU | 30 | Fuel Level Sensor Signal
E | 0.5 BK/YE | 2709 | 5 Volt Reference 1 | E | 0.5 BK/YE | 2709 | 5 Volt Reference 1
F | 0.5 BU/WH | 890 | Fuel Tank Pressure Sensor Signal | F | 0.5 BU/WH | 890 | Fuel Tank Pressure Sensor Signal
G | 0.5 BK/GN | 2759 | Low Reference | G | 0.5 BK/GN | 2759 | Low Reference
H | 0.5 BK/BN | 474 | 5 Volt Reference 1 | H | 0.5 BK/BN | 474 | 5 Volt Reference 1
J | 0.5 GN/BN | 5266 | Ambient Air Pressure Sensor Signal | J | 0.5 GN/BN | 5266 | Ambient Air Pressure Sensor Signal
K | 0.5 GN/BK | 6014 | Low Reference | K | 0.5 GN/BK | 6014 | Low Reference
L | 1 BU | 5372 | Ignition Voltage | L | 1 BU | 5372 | Ignition Voltage
M | 1 BN | 2350 | EVAP Canister Vent Solenoid Control | M | 1 BN | 2350 | EVAP Canister Vent Solenoid Control

### X401 Liftgate Extension Harness to Rear Body Harness

#### Connector Part Information

- OEM: 30234001
- Service: Service by Harness - See Part Catalog
- Description: 11-Way F (GY)

#### Connector Part Information

- OEM: 30331101
- Service: Service by Harness - See Part Catalog
- 11-Way M 1.5, 5.8 Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X401 Liftgate Extension Harness to Rear Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/YE | 5797 | Rear Closure Handle Switch Open Signal | 1 | 0.5 BU/YE | 5797 | Rear Closure Handle Switch Open Signal
2 | 0.75 BN/WH | 5799 | Lift Gate Open/Close Motor Close Control | 2 | 0.75 BN/WH | 5799 | Lift Gate Open/Close Motor Close Control
3 | 0.5 BK/BU | 1303 | Liftgate Ajar Switch Signal | 3 | 0.5 BK/BU | 1303 | Liftgate Ajar Switch Signal
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.5 BK/YE | 820 | CHMSL Supply Voltage | 5 | 0.5 BK/YE | 820 | CHMSL Supply Voltage
6 | 1.5 BK | 1939 | Run/Crank Ignition 1 Voltage | 6 | 1.5 BK | 1939 | Run/Crank Ignition 1 Voltage
7 | 1.5 BU | 393 | Rear Window Wiper Motor Control | 7 | 1.5 BU | 393 | Rear Window Wiper Motor Control
8-9 | -- | -- | Not Used | 8-9 | -- | -- | Not Used
10 | 4 BN | 2550 | Ground | 10 | 4 BN | 2550 | Ground
11 | 2.5 BK | 293 | Rear Defog Element Supply Voltage | 11 | 2.5 BK | 293 | Rear Defog Element Supply Voltage

### X402 Rear Facia Harness to Body Rear Harness

#### Connector Part Information

- OEM: 1452327-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F 2.8 Junior Power Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 1452324-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way M 2.8 Junior Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X402 Rear Facia Harness to Body Rear Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 GY/GN | 1255 | Side Marker Supply Voltage Signal | 1 | 0.5 GY/GN | 1255 | Side Marker Supply Voltage Signal
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | 0.5 BN | 2550 | Ground | 3 | 0.5 BN | 2550 | Ground
4-5 | -- | -- | Not Used | 4-5 | -- | -- | Not Used
6 | 0.5 GY/GN | 1255 | Side Marker/License Supply Voltage Signal | 6 | 0.5 GY/GN | 1255 | License Supply Voltage Signal

### X403 Rear Axle ABS Harness to Body Harness

#### Connector Part Information

- OEM: 1452327-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Junior Power Timer Series, Sealed (BK)

#### Connector Part Information

- OEM: 1452324-1
- Service: 93185233
- Description: 6-Way M 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93185233
- Release Tool/Test Probe: N/A

#### X403 Rear Axle ABS Harness to Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BN/RD | 883 | Low Reference | 1 | 0.5 BN/RD | 883 | Low Reference
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | 0.5 BN/BU | 885 | Low Reference | 3 | 0.5 BN/BU | 885 | Low Reference
4 | 0.5 BU/RD | 882 | Wheel Speed Sensor Signal Right Rear | 4 | 0.5 BU/RD | 882 | Wheel Speed Sensor Signal Right Rear
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 BU | 884 | Wheel Speed Sensor Signal Left Rear | 6 | 0.5 BU | 884 | Wheel Speed Sensor Signal Left Rear

### X500 Body Harness to Driver Door Harness

#### Connector Part Information

- OEM: 30432421
- Service: 93191096
- Description: 34-Way F 1.5, 2.8 Series, Sealed (BK)

#### Connector Part Information

- OEM: 30530621
- Service: Service by Harness - See Part Catalog
- Description: 34-Way M 1.5, 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X500 Body Harness to Driver Door Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.5 RD | 2040 | Battery Positive Voltage | 1 | 2.5 RD | 2040 | Battery Positive Voltage
2 | 2.5 BN | 1550 | Ground | 2 | 2.5 BN | 1550 | Ground
3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal | 3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal | 4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 WH/GY | 49 | Driver Door Ajar Switch Signal | 6 | 0.5 WH/GY | 49 | Driver Door Ajar Switch Signal
7 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal | 7 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal
8 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal | 8 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal
9 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal | 9 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal
10 | 0.75 BU | 201 | Left Front Speaker (+) | 10 | 0.75 BU | 201 | Left Front Speaker (+)
11 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-) | 11 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-)
12 | 0.5 BU/BK | 6162 | Outside Right Mirror Vertical Position Control | 12 | 0.5 BU/BK | 6162 | Outside Right Mirror Vertical Position Control
13 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire | 13 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire
14 | 0.5 GN/BK | 6161 | Outside Right Mirror Horizontal Position Control | 14 | 0.5 GN/BK | 6161 | Outside Right Mirror Horizontal Position Control
15 | 0.75 WH/BK | 2267 | Mirror Heating Element Supply Voltage | 15 | 0.75 WH/BK | 2267 | Mirror Heating Element Supply Voltage
16 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal (5 Door) | 16 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal (5 Door)
17 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal (5 Door) | 17 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal (5 Door)
18 | 0.5 BK | 4 | Accessory Voltage | 18 | 0.5 BK | 4 | Accessory Voltage
19 | 0.5 BU/GN | 170 | Power Window Master Switch Right Rear Up Signal (5 Door) | 19 | 0.5 BU/GN | 170 | Power Window Master Switch Right Rear Up Signal (5 Door)
20 | 0.5 BU/BN | 171 | Power Window Master Switch Right Rear Down Signal (5 Door) | 20 | 0.5 BU/BN | 171 | Power Window Master Switch Right Rear Down Signal (5 Door)
21 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal (5 Door) | 21 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal (5 Door)
22-34 | -- | -- | Not Used | 22-34 | -- | -- | Not Used

### X600 Body Harness to Passenger Door Harness

#### Connector Part Information

- OEM: 30432421
- Service: 93191096
- Description: 34-Way F 1.5, 2.8 Series, Sealed (BK)

#### Connector Part Information

- OEM: 30530621
- Service: Service by Harness - See Part Catalog
- Description: 34-Way M 1.5, 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X600 Body Harness to Passenger Door Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.5 RD | 2140 | Battery Positive Voltage | 1 | 2.5 RD | 2140 | Battery Positive Voltage
2 | 2.5 BN | 2050 | Ground | 2 | 2.5 BN | 2050 | Ground
3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal | 3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal | 4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 GY | 746 | Right Front Door Ajar Switch Signal | 6 | 0.5 GY | 746 | Right Front Door Ajar Switch Signal
7 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal | 7 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal
8 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal | 8 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal
9 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal | 9 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal
10 | 0.75 YE | 200 | Right Front Speaker (+) | 10 | 0.75 YE | 200 | Right Front Speaker (+)
11 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-) | 11 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-)
12 | 0.5 BU/BK | 6162 | Outside Right Mirror Vertical Position Control | 12 | 0.5 BU/BK | 6162 | Outside Right Mirror Vertical Position Control
13 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire | 13 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire
14 | 0.5 GN/BK | 6161 | Outside Right Mirror Horizontal Position Control | 14 | 0.5 GN/BK | 6161 | Outside Right Mirror Horizontal Position Control
15 | 0.75 WH/BK | 2267 | Mirror Heating Element Supply Voltage | 15 | 0.75 WH/BK | 2267 | Mirror Heating Element Supply Voltage
16-17 | -- | -- | Not Used | 16-17 | -- | -- | Not Used
18 | 0.5 BK | 4 | Accessory Voltage | 18 | 0.5 BK | 4 | Accessory Voltage
19-34 | -- | -- | Not Used | 19-34 | -- | -- | Not Used

### X700 Body Harness to Left Rear Door Harness (5 Door)

#### Connector Part Information

- OEM: 15345078
- Service: 93189351
- Description: 19-Way F Mixed Series, Sealed (BK)

#### Connector Part Information

- OEM: 15446405
- Service: Service by Harness - See Part Catalog
- Description: 19-Way M Mixed Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X700 Body Harness to Left Rear Door Harness (5 Door)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.5 RD | 2240 | Battery Positive Voltage | 1 | 2.5 RD | 2240 | Battery Positive Voltage
2 | 2.5 BN | 2350 | Ground | 2 | 2.5 BN | 2350 | Ground
3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal | 3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal | 4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 GY | 747 | Left Rear Door Ajar Switch Signal | 6 | 0.5 GY | 747 | Left Rear Door Ajar Switch Signal
6 | 0.5 GY | 747 | Left Rear Door Ajar Switch Signal | 6 | 0.5 GY | 747 | Left Rear Door Ajar Switch Signal
7 | -- | -- | Not Used | 12 | -- | -- | Not Used
8 | -- | -- | Not Used | 11 | -- | -- | Not Used
9 | -- | -- | Not Used | 10 | -- | -- | Not Used
10 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal | 9 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal
11 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal | 8 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal
12 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal | 7 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal
13 | -- | -- | Not Used | 19 | -- | -- | Not Used
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | -- | -- | Not Used | 17 | -- | -- | Not Used
16 | 0.75 GN | 199 | Left Rear Speaker (+) | 16 | 0.75 GN | 199 | Left Rear Speaker (+)
17 | 0.75 BN/GN | 116 | Left Rear Speaker Signal (-) | 15 | 0.75 BN/GN | 116 | Left Rear Speaker Signal (-)
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal | 13 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal

### X800 Body Harness to Right Rear Door Harness (5 Door)

#### Connector Part Information

- OEM: 15345078
- Service: 93189351
- Description: 19-Way F Mixed Series, Sealed (BK)

#### Connector Part Information

- OEM: 15446405
- Service: Service by Harness - See Part Catalog
- Description: 19-Way M Mixed Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X800 Body Harness to Right Rear Door Harness (5 Door)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.5 RD | 2340 | Battery Positive Voltage | 1 | 2.5 RD | 2340 | Battery Positive Voltage
2 | 2.5 BN | 2050 | Ground | 2 | 2.5 BN | 2350 | Ground
3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal | 3 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal | 4 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.5 GY | 748 | Right Rear Door Ajar Switch Signal | 6 | 0.5 GY | 748 | Right Rear Door Ajar Switch Signal
7 | -- | -- | Not Used | 12 | -- | -- | Not Used
8 | -- | -- | Not Used | 11 | -- | -- | Not Used
9 | -- | -- | Not Used | 10 | -- | -- | Not Used
10 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal | 9 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal
11 | 0.5 BU/GN | 170 | Power Window Master Switch Right Rear Up Signal | 8 | 0.5 VT/GN | 168 | Power Window Master Switch Right Rear Up Signal
12 | 0.5 BU/BN | 171 | Power Window Master Switch Right Rear Down Signal | 7 | 0.5 VT/BN | 169 | Power Window Master Switch Right Rear Down Signal
13 | -- | -- | Not Used | 19 | -- | -- | Not Used
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | -- | -- | Not Used | 17 | -- | -- | Not Used
16 | 0.75 WH | 46 | Right Rear Speaker (+) | 16 | 0.75 GN | 199 | Right Rear Speaker (+)
17 | 0.75 BN/WH | 115 | Right Rear Speaker Signal (-) | 15 | 0.75 BN/WH | 115 | Right Rear Speaker Signal (-)
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal | 13 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal

### X901 Liftgate Extension Harness to Liftgate Harness

#### Connector Part Information

- OEM: 30234001
- Service: Service by Harness - See Part Catalog
- Description: 11-Way F (BK)

#### Connector Part Information

- OEM: 30331101
- Service: Service by Harness - See Part Catalog
- 11-Way M 1.5, 5.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### X901 Liftgate Jumper Harness to Liftgate Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BU/YE | 5797 | Rear Closure Handle Switch Open Signal | 1 | 0.5 BU/YE | 5797 | Rear Closure Handle Switch Open Signal
2 | 0.75 BN/WH | 5799 | Lift Gate Open/Close Motor Close Control | 2 | 0.75 BN/WH | 5799 | Lift Gate Open/Close Motor Close Control
3 | 0.5 BK/BU | 1303 | Liftgate Ajar Switch Signal | 3 | 0.5 BK/BU | 1303 | Liftgate Ajar Switch Signal
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.5 BK/YE | 820 | CHMSL Supply Voltage | 5 | 0.5 BK/YE | 820 | CHMSL Supply Voltage
6 | 1.5 BK | 1939 | Run/Crank Ignition 1 Voltage | 6 | 1.5 BK | 1939 | Run/Crank Ignition 1 Voltage
7 | 1.5 BU | 393 | Rear Window Wiper Motor Control | 7 | 1.5 BU | 393 | Rear Window Wiper Motor Control
8-9 | -- | -- | Not Used | 8-9 | -- | -- | Not Used
10 | 4 BN | 2550 | Ground | 10 | 4 BN | 2550 | Ground
11 | 2.5 BK | 293 | Rear Defog Element Supply Voltage | 11 | 2.5 BK | 293 | Rear Defog Element Supply Voltage