For 1990-2009 cars

### Removal Procedure

1. Open the driver door.
2. Remove the instrument panel (I/P) insulator panel. Refer to Instrument Panel Insulator Panel Replacement .
3. Disconnect the wiring harness plug (1).

Remove the wiring harness plug in the direction of the arrow.

4. Remove the accelerator pedal position sensor.

Remove and discard the 3 nuts (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the accelerator pedal position sensor.

Use NEW nuts.

Tighten
Tighten the 3 nuts to 12 N·m (106 lb in).

2. Install the wiring harness plug.
3. Install the I/P insulator panel. Refer to Instrument Panel Insulator Panel Replacement .
4. Close the driver door.